V 10
1
LANG:5 8 (NoName)
PANEL,299 141 462 272 N {204,153,204} 0
EEE E E 1 -1 -1 0  10 10
"" 0 1
EE 2
"CBRef""1"
"EClose"E
""
DISPLAY_LAYER, 1 0 1 0 1 0 1 0 1 0 1 0 1 0 1 0
LAYER, 0 
1
LANG:5 6 Layer1
2 2
"Text2"
""
1 10 10 E E E 1 E 1 E N {0,0,0} E N {239,222,239} E E
 E E
3 0 0 0 0 0
EE E
0
1
LANG:5 0 
1
"dashclr"N "_Transparent"
E E 0 1 1 0 1 E U  1 E 12 12 448 248
0 2 0 "s" 0 0 0 64 0 0  12 12
 16
1
LANG:5 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:5 35 A failure shall be indicated when: 
1
LANG:5 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:5 63 1) Output voltage is low and the unit is not in current limit. 
1
LANG:5 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:5 56 2) An over- temperature condition has caused the uit to 
1
LANG:5 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:5 11 shut down. 
1
LANG:5 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:5 54 3) An OVP condition has caused the unit to shut down. 
1
LANG:5 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:5 59 4) The primary side boost converter (PFC) output voltage is
1
LANG:5 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:5 49 low when the AC voltage is within specification. 
1
LANG:5 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:5 53 5) The AC line has not yet been applied to the unit. 
1
LANG:5 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:5 60 6) The AC line voltage is too low to operate the bias supply
1
LANG:5 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:5 62 and therefore the relay coil has insufficient voltage to keep 
1
LANG:5 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:5 20 the contacts closed.
1
LANG:5 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:5 0 
1
LANG:5 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:5 28 FALSE: Power supply failure 
1
LANG:5 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:5 0 
1
LANG:5 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:5 22 TRUE: Normal operation
1
LANG:5 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:5 0 
0
LAYER, 1 
1
LANG:5 6 Layer2
0
LAYER, 2 
1
LANG:5 6 Layer3
0
LAYER, 3 
1
LANG:5 6 Layer4
0
LAYER, 4 
1
LANG:5 6 Layer5
0
LAYER, 5 
1
LANG:5 6 Layer6
0
LAYER, 6 
1
LANG:5 6 Layer7
0
LAYER, 7 
1
LANG:5 6 Layer8
0
0