V 10
1
LANG:1 8 (NoName)
PANEL,347 85 1214 815 N "_3DFace" 0
EEE E E 1 -1 -1 0  130 90
"" 0 1
E"//Getting Colour
//%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
EP_setBackColorE(string dpSource, float temperature)
{
int limit, channelnb;

//DebugN(dpSource,temperature );

 dpGet(\"SCTmops1:Limit.Indx\", limit);
   
  if (dpSource == \"Crate00.Channel100.MOch_Tm0.Recv:_online.._value\")
    setValue(\"\", \"backCol\", \"_InputFieldBackground\");
    
  else if (dpSource == \"Crate00.Channel100.MOch_Tm1.Recv:_online.._value\")
    setValue(\"\", \"backCol\", \"_InputFieldBackground\");
    
  else {
      setValue(\"\", \"backCol\", \"\"); 
      if (temperature > limit)
          setValue(\"\", \"backCol\", \"Red\");
      else
          setValue(\"\", \"backCol\", \"\");  
      }
}


//Getting Value
//%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
EP_textFieldIn22(string DPstavenb, int stavenb)
{
dyn_errClass err;
//string* datapoint1;
string datapoint,dp1;
int i;
int crate,count;
string channel;



dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(DPstavenb, stavenb);
channel=\"SCTmops1:Sector.Row_00.ST_00:_online.._value\";

sprintf(datapoint, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, stavenb);

if( dpSubStr( datapoint, DPSUB_DP_EL ) == \"\" )
  {
    setValue(\"\", \"color\", \"_dpdoesnotexist\");
    return;
  }
   dpConnect(\"EP_textFieldInCB\",channel, DPstavenb);

count=47;
for(i=0; i<= count;i++)
  {
  sprintf(datapoint,\"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate,i);
  dpConnect(\"EP_textFieldInCB1\",datapoint, DPstavenb);  
  }                   
 err = getLastError();
 if (dynlen(err) > 0)
 setValue(\"\", \"color\", \"_dpdoesnotexist\");
}

EP_textFieldInCB(string dp, float fNewValue, string DPstavenb, int stavenb)
{ 
int crate;
int hv;
float a,b,t,x;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
//dpGet(DPstage, hv);
sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, stavenb);
dpGet(dp1,fNewValue);

sprintf(sTmp,\"%f\",fNewValue);
setValue(\"\", \"text\", fNewValue );
EP_setBackColor(dp1,fNewValue);
}

EP_textFieldInCB1(string dp, float fNewValue, string DPstavenb, int stavenb)
{ 
int crate;
int hv;
float a,b,t,x;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
//dpGet(\"SCTmops1:Sector.Row_00.ST_00:_online.._value\", hv);
sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, stavenb);
dpGet(dp1,fNewValue);


sprintf(sTmp,\"%f\",fNewValue);
setValue(\"\", \"text\", fNewValue );
EP_setBackColor(dp1,fNewValue);

}
" 0
 2
"CBRef""1"
"EClose"E
""
DISPLAY_LAYER, 1 0 1 0 1 0 1 0 1 0 1 0 1 0 1 0
LAYER, 0 
1
LANG:1 6 Layer1
30 597
"Frame1"
""
1 77 721 E E E 1 E 1 E N "_3DText" E N "_Transparent" E E
 E E
596 0 0 0 0 0
EE E
1
1
LANG:1 0 
0
E E 0 1 1 0 1 E U  0 E 77 50 571 721
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-140-100-100-*-*-iso8859-1|-15,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 11 Module - LV
2 96
"Text97"
""
1 200 15 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
97 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
E E 0 1 1 0 1 E U  1 E 202 17 376 39
0 2 0 "s" 0 0 0 192 0 0  202 17
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-160-100-100-*-*-iso8859-1|-19,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 15 SECTOR - VALUES
30 265
"Frame5"
""
1 90 700 E E E 1 E 1 E N "_3DText" E N "_Transparent" E E
 E E
264 0 0 0 0 0
EE E
2
1
LANG:1 0 
0
E E 0 1 1 0 1 E U  0 E 90 570 220 700
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 14 Dynamic Limits
2 268
"Text51"
""
1 110 600 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
267 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
E E 0 1 1 0 1 E U  1 E 112 602 189 617
0 2 0 "s" 0 0 0 192 0 0  112 602
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 11 Temperature
2 269
"Text52"
""
1 123 663 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
268 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
E E 0 1 1 0 1 E U  1 E 125 665 174 680
0 2 0 "s" 0 0 0 192 0 0  125 665
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 7 Current
2 272
"Text54"
""
1 197 630 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
271 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
E E 0 1 1 0 1 E U  1 E 199 632 206 647
0 2 0 "s" 0 0 0 192 0 0  199 632
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 1 C
2 559
"Text17"
""
1 162 96 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
558 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_00:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_00:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Vcc.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vcc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_00:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vcc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 164 98 200 114
1 2 0 "s" 0 0 0 64 0 0  164 98
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Vcc
2 561
"Text71"
""
1 162 68 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
560 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
E E 0 1 1 0 1 E U  1 E 164 70 207 83
0 2 0 "s" 0 0 0 64 0 0  164 70
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 7 Vcc (V)
2 562
"Text72"
""
1 212 68 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
561 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
E E 0 1 1 0 1 E U  1 E 214 70 258 83
0 2 0 "s" 0 0 0 64 0 0  214 70
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 Vdd (V) 
2 563
"Text73"
""
1 263 68 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
562 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
E E 0 1 1 0 1 E U  1 E 265 70 310 86
0 2 0 "s" 0 0 0 64 0 0  265 70
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 5 VCSEL
2 564
"Text74"
""
1 316 68 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
563 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
E E 0 1 1 0 1 E U  1 E 318 70 394 86
0 2 0 "s" 0 0 0 64 0 0  318 70
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 PIN Bias
2 566
"Text76"
""
1 369 68 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
565 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
E E 0 1 1 0 1 E U  1 E 371 70 417 83
0 2 0 "s" 0 0 0 64 0 0  371 70
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 9 Icc (mA) 
2 567
"Text77"
""
1 471 68 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
566 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
E E 0 1 1 0 1 E U  1 E 473 70 539 86
0 2 0 "s" 0 0 0 64 0 0  473 70
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 9 T L0 (C) 
2 568
"Text78"
""
1 522 68 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
567 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
E E 0 1 1 0 1 E U  1 E 524 70 588 84
0 2 0 "s" 0 0 0 64 0 0  524 70
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 T L1 (C)
2 570
"Text42"
""
1 82 95 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
569 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_00:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_00:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_00:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 84 97 108 114
1 2 0 "s" 0 0 0 64 0 0  84 97
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 LVchStat
2 571
"Text43"
""
1 80 69 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
570 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
E E 0 1 1 0 1 E U  1 E 82 71 128 84
0 2 0 "s" 0 0 0 64 0 0  82 71
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 6 Status
2 572
"Text44"
""
1 122 95 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
571 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"// SimpleCtrlScriptStart {invalid}
main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_00:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_00:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,xTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);

  
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
  // EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

sprintf(xTmp,\"%x\", temperature);
setValue(\"\", \"text\", xTmp);

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,xTmp;

//EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
sprintf(xTmp,\"%x\", temperature);
setValue(\"\", \"text\", xTmp);
//setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_00:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   //EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}


// SimpleCtrlScript {EP_textFieldIn}
// DP {Crate1.HVchVolt}
// DPConfig {:_online.._value}
// DPType {float}
// UseDPUnit {TRUE}
// UseDPFormat {TRUE}
// SimpleCtrlScriptEnd {EP_textFieldIn}
" 0
 E 0 1 1 0 1 E U  1 E 124 97 148 114
1 2 0 "s" 0 0 0 64 0 0  124 97
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 LVchStat
2 585
"Text20"
""
1 370 96 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
584 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_00:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_00:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Icc.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Icc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_00:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Icc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 372 98 408 114
1 2 0 "s" 0 0 0 64 0 0  372 98
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Icc
2 586
"Text21"
""
1 214 96 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
585 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_00:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_00:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Vdd.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vdd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_00:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vdd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 216 98 252 114
1 2 0 "s" 0 0 0 64 0 0  216 98
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Vdd
2 588
"Text24"
""
1 422 96 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
587 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_00:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_00:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Idd.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Idd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_00:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Idd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 424 98 460 114
1 2 0 "s" 0 0 0 64 0 0  424 98
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Idd
2 589
"Text25"
""
1 266 96 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
588 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_00:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_00:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchVCSL.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchVCSL.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_00:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchVCSL.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 268 98 304 114
1 2 0 "s" 0 0 0 64 0 0  268 98
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVchVCSV
2 591
"Text27"
""
1 318 96 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
590 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_00:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_00:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchPINV.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchPINV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_00:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchPINV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 320 98 356 114
1 2 0 "s" 0 0 0 64 0 0  320 98
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVchPINV
2 593
"Text29"
""
1 474 96 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
592 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_00:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_00:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
if (channelnb==100) {
   temperature=-28; 
   EP_setBackColorE(dp1,temperature);
   }
else {   
   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);
   }
//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_00:_online.._value\", channelnb);

if (channelnb==100) {
   temperature=-28; 
   EP_setBackColorE(dp1,temperature);
   }
else { 
   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   }
//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 476 98 512 114
1 2 0 "s" 0 0 0 64 0 0  476 98
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 MOch_Tm0
2 594
"Text30"
""
1 526 96 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
593 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_00:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_00:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_00:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 528 98 564 114
1 2 0 "s" 0 0 0 64 0 0  528 98
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 MOch_Tm1
30 603
"Frame3"
""
1 573 720 E E E 1 E 1 E N "_3DText" E N "_Transparent" E E
 E E
602 0 0 0 0 0
EE E
1
1
LANG:1 0 
0
E E 0 1 1 0 1 E U  0 E 573 49 790 720
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-140-100-100-*-*-iso8859-1|-15,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 11 Module - HV
2 604
"Text10"
""
1 713 96 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
603 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_00:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_00:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchCurr.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchCurr.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_00:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchCurr.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 715 98 781 114
1 2 0 "s" 0 0 0 64 0 0  715 98
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 HVchCurr
2 607
"Text99"
""
1 659 69 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
606 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
E E 0 1 1 0 1 E U  1 E 661 71 727 84
0 2 0 "s" 0 0 0 64 0 0  661 71
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 Volt (V)
2 608
"Text1"
""
1 583 95 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
607 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_00:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_00:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
if (channelnb==100) {
   temperature=-28; 
 //  EP_setBackColorE(dp1,temperature);
   }
else {   
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   //EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);
   }
//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

//EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_00:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
  // EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 585 97 609 114
1 2 0 "s" 0 0 0 64 0 0  585 97
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 HVchStat
2 609
"Text5"
""
1 579 69 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
608 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
E E 0 1 1 0 1 E U  1 E 581 71 627 84
0 2 0 "s" 0 0 0 64 0 0  581 71
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 6 Status
2 610
"Text9"
""
1 623 77 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
609 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_00:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_00:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,xTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);

  
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
  // EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

sprintf(xTmp,\"%x\", temperature);
setValue(\"\", \"text\", xTmp);

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,xTmp;

//EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
sprintf(xTmp,\"%x\", temperature);
setValue(\"\", \"text\", xTmp);
//setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_00:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   //EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}
" 0
 E 0 1 1 0 1 E U  1 E 625 97 647 114
1 2 0 "s" 0 0 0 64 0 0  625 97
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 HVchStat
2 612
"Text12"
""
1 661 96 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
611 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_00:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_00:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchVolt.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchVolt.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_00:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchVolt.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 663 98 699 114
1 2 0 "s" 0 0 0 64 0 0  663 98
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 HVchVolt
2 614
"Text6"
""
1 419 68 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
613 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
E E 0 1 1 0 1 E U  1 E 421 70 467 83
0 2 0 "s" 0 0 0 64 0 0  421 70
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 9 Idd (mA) 
2 606
"Text98"
""
1 710 69 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
605 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
E E 0 1 1 0 1 E U  1 E 712 71 758 84
0 2 0 "s" 0 0 0 64 0 0  712 71
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 7 Current
2 611
"Text16"
""
1 755 69 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
610 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
E E 0 1 1 0 1 E U  1 E 757 71 783 88
0 2 0 "s" 0 0 0 64 0 0  757 71
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 5 ( nA)
2 782
"Text2"
""
1 162 122 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
781 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_01:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_01:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Vcc.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vcc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_01:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vcc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 164 124 200 140
1 2 0 "s" 0 0 0 64 0 0  164 124
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Vcc
2 783
"Text3"
""
1 82 121 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
782 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_01:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_01:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_01:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 84 123 108 140
1 2 0 "s" 0 0 0 64 0 0  84 123
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 LVchStat
2 784
"Text4"
""
1 122 121 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
783 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_01:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_01:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_01:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 124 123 148 140
1 2 0 "s" 0 0 0 64 0 0  124 123
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 LVchStat
2 785
"Text7"
""
1 370 122 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
784 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_01:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_01:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Icc.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Icc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_01:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Icc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 372 124 408 140
1 2 0 "s" 0 0 0 64 0 0  372 124
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Icc
2 786
"Text8"
""
1 214 122 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
785 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_01:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_01:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Vdd.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vdd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_01:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vdd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 216 124 252 140
1 2 0 "s" 0 0 0 64 0 0  216 124
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Vdd
2 787
"Text11"
""
1 422 122 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
786 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_01:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_01:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Idd.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Idd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_01:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Idd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 424 124 460 140
1 2 0 "s" 0 0 0 64 0 0  424 124
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Idd
2 788
"Text13"
""
1 266 122 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
787 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_01:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_01:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchVCSV.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchVCSV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_01:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchVCSV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 268 124 304 140
1 2 0 "s" 0 0 0 64 0 0  268 124
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVchVCSV
2 789
"Text14"
""
1 318 122 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
788 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_01:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_01:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchPINV.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchPINV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_01:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchPINV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 320 124 356 140
1 2 0 "s" 0 0 0 64 0 0  320 124
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVchPINV
2 790
"Text15"
""
1 474 122 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
789 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_01:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_01:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_01:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 476 124 512 140
1 2 0 "s" 0 0 0 64 0 0  476 124
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 MOch_Tm0
2 791
"Text18"
""
1 526 122 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
790 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_01:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_01:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_01:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 528 124 564 140
1 2 0 "s" 0 0 0 64 0 0  528 124
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 MOch_Tm1
2 792
"Text19"
""
1 713 122 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
791 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_01:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_01:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchCurr.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchCurr.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_01:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchCurr.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 715 124 781 140
1 2 0 "s" 0 0 0 64 0 0  715 124
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 HVchCurr
2 793
"Text22"
""
1 583 121 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
792 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_01:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_01:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_01:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 585 123 609 140
1 2 0 "s" 0 0 0 64 0 0  585 123
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 HVchStat
2 794
"Text23"
""
1 623 103 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
793 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_01:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_01:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_01:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 625 123 647 140
1 2 0 "s" 0 0 0 64 0 0  625 123
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 HVchStat
2 795
"Text26"
""
1 661 122 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
794 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_01:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_01:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchVolt.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchVolt.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_01:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchVolt.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 663 124 699 140
1 2 0 "s" 0 0 0 64 0 0  663 124
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 HVchVolt
2 797
"Text28"
""
1 162 152 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
796 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_02:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_02:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Vcc.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vcc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_02:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vcc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 164 154 200 170
1 2 0 "s" 0 0 0 64 0 0  164 154
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Vcc
2 798
"Text31"
""
1 82 151 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
797 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_02:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_02:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_02:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 84 153 108 170
1 2 0 "s" 0 0 0 64 0 0  84 153
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 LVchStat
2 799
"Text32"
""
1 122 151 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
798 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_02:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_02:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_02:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 124 153 148 170
1 2 0 "s" 0 0 0 64 0 0  124 153
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 LVchStat
2 800
"Text33"
""
1 370 152 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
799 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_02:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_02:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Icc.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Icc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_02:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Icc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 372 154 408 170
1 2 0 "s" 0 0 0 64 0 0  372 154
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Icc
2 801
"Text34"
""
1 214 152 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
800 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_02:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_02:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Vdd.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vdd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_02:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vdd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 216 154 252 170
1 2 0 "s" 0 0 0 64 0 0  216 154
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Vdd
2 802
"Text35"
""
1 422 152 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
801 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_02:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_02:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Idd.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Idd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_02:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Idd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 424 154 460 170
1 2 0 "s" 0 0 0 64 0 0  424 154
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Idd
2 803
"Text36"
""
1 266 152 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
802 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_02:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_02:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchVCSV.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchVCSV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_02:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchVCSV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 268 154 304 170
1 2 0 "s" 0 0 0 64 0 0  268 154
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVchVCSV
2 804
"Text37"
""
1 318 152 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
803 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_02:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_02:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchPINV.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchPINV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_02:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchPINV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 320 154 356 170
1 2 0 "s" 0 0 0 64 0 0  320 154
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVchPINV
2 805
"Text38"
""
1 474 152 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
804 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_02:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_02:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_02:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 476 154 512 170
1 2 0 "s" 0 0 0 64 0 0  476 154
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 MOch_Tm0
2 806
"Text39"
""
1 526 152 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
805 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_02:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_02:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_02:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 528 154 564 170
1 2 0 "s" 0 0 0 64 0 0  528 154
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 MOch_Tm1
2 807
"Text40"
""
1 713 152 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
806 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_02:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_02:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchCurr.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchCurr.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_02:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchCurr.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 715 154 781 170
1 2 0 "s" 0 0 0 64 0 0  715 154
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 HVchCurr
2 808
"Text41"
""
1 583 151 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
807 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_02:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_02:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_02:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 585 153 609 170
1 2 0 "s" 0 0 0 64 0 0  585 153
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 HVchStat
2 809
"Text45"
""
1 623 133 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
808 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_02:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_02:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_02:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 625 153 647 170
1 2 0 "s" 0 0 0 64 0 0  625 153
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 HVchStat
2 810
"Text46"
""
1 661 152 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
809 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_02:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_02:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchVolt.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchVolt.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_02:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchVolt.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 663 154 699 170
1 2 0 "s" 0 0 0 64 0 0  663 154
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 HVchVolt
2 813
"Text48"
""
1 162 182 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
812 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"// SimpleCtrlScriptStart {invalid}
main()
{
  EP_textFieldIn();
  EP_setInvalid();
}

EP_textFieldIn()
{
dyn_errClass err;

  if( dpSubStr( \"SCTmops1:Sector.Row_00.ST_03:_online.._value\", DPSUB_DP_EL ) == \"\" )
  {
    setValue(\"\", \"color\", \"_dpdoesnotexist\");
    return;
  }

  dpConnect(\"EP_textFieldInCB\",
            \"SCTmops1:Sector.Row_00.ST_03:_online.._value\");
  err = getLastError();
  if (dynlen(err) > 0)
    setValue(\"\", \"color\", \"_dpdoesnotexist\");

}


EP_textFieldInCB(string dp, int iNewValue)
{
  setValue(\"\", \"text\", iNewValue);
}

EP_setInvalid()
{
dyn_errClass err;

  if( dpSubStr( \"SCTmops1:Sector.Row_00.ST_03:_online.._invalid\", DPSUB_DP_EL ) == \"\" )
  {
    setValue(\"\", \"color\", \"_dpdoesnotexist\");
    return;
  }

  dpConnect(\"EP_setInvalidCB\",
            \"SCTmops1:Sector.Row_00.ST_03:_online.._invalid\");
  err = getLastError();
  if (dynlen(err) > 0)
    setValue(\"\", \"color\", \"_dpdoesnotexist\");

}

EP_setInvalidCB(string dp, bool boInvalid)
{
  setValue(\"\", \"color\", (boInvalid ? \"_invalid\" : \"\"));
}

// SimpleCtrlScript {EP_textFieldIn}
// DP {SCTmops1:Sector.Row_00.ST_03}
// DPConfig {:_online.._value}
// DPType {int}
// UseDPUnit {FALSE}
// UseDPFormat {FALSE}
// SimpleCtrlScriptEnd {EP_textFieldIn}
// SimpleCtrlScript {EP_setInvalid}
// DP {SCTmops1:Sector.Row_00.ST_03}
// DPConfig {:_online.._invalid}
// DPType {bool}
// Attribut {color}
// SimpleCtrlScriptEnd {EP_setInvalid}
" 0
 E 0 1 1 0 1 E U  1 E 164 184 200 200
1 2 0 "s" 0 0 0 64 0 0  164 184
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Vcc
2 814
"Text49"
""
1 82 181 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
813 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 84 183 108 200
1 2 0 "s" 0 0 0 64 0 0  84 183
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 LVchStat
2 815
"Text50"
""
1 122 181 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
814 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 124 183 148 200
1 2 0 "s" 0 0 0 64 0 0  124 183
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 LVchStat
2 816
"Text53"
""
1 370 182 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
815 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Icc.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Icc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Icc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 372 184 408 200
1 2 0 "s" 0 0 0 64 0 0  372 184
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Icc
2 817
"Text55"
""
1 214 182 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
816 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Vdd.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vdd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vdd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 216 184 252 200
1 2 0 "s" 0 0 0 64 0 0  216 184
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Vdd
2 818
"Text56"
""
1 422 182 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
817 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Idd.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Idd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Idd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 424 184 460 200
1 2 0 "s" 0 0 0 64 0 0  424 184
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Idd
2 819
"Text57"
""
1 266 182 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
818 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchVCSV.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchVCSV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchVCSV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 268 184 304 200
1 2 0 "s" 0 0 0 64 0 0  268 184
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVchVCSV
2 820
"Text58"
""
1 318 182 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
819 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchPINV.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchPINV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchPINV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 320 184 356 200
1 2 0 "s" 0 0 0 64 0 0  320 184
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVchPINV
2 821
"Text59"
""
1 474 182 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
820 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 476 184 512 200
1 2 0 "s" 0 0 0 64 0 0  476 184
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 MOch_Tm0
2 822
"Text60"
""
1 526 182 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
821 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 528 184 564 200
1 2 0 "s" 0 0 0 64 0 0  528 184
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 MOch_Tm1
2 823
"Text61"
""
1 713 182 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
822 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchCurr.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchCurr.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchCurr.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 715 184 781 200
1 2 0 "s" 0 0 0 64 0 0  715 184
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 HVchCurr
2 824
"Text62"
""
1 583 181 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
823 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 585 183 609 200
1 2 0 "s" 0 0 0 64 0 0  585 183
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 HVchStat
2 825
"Text63"
""
1 623 163 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
824 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 625 183 647 200
1 2 0 "s" 0 0 0 64 0 0  625 183
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 HVchStat
2 826
"Text64"
""
1 661 182 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
825 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchVolt.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchVolt.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchVolt.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 663 184 699 200
1 2 0 "s" 0 0 0 64 0 0  663 184
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 HVchVolt
2 828
"Text65"
""
1 162 212 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
827 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_04:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_04:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Vcc.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vcc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_04:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vcc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 164 214 200 230
1 2 0 "s" 0 0 0 64 0 0  164 214
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Vcc
2 829
"Text66"
""
1 82 211 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
828 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 84 213 108 230
1 2 0 "s" 0 0 0 64 0 0  84 213
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 LVchStat
2 830
"Text67"
""
1 122 211 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
829 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 124 213 148 230
1 2 0 "s" 0 0 0 64 0 0  124 213
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 LVchStat
2 831
"Text68"
""
1 370 212 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
830 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Icc.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Icc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Icc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 372 214 408 230
1 2 0 "s" 0 0 0 64 0 0  372 214
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Icc
2 832
"Text69"
""
1 214 212 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
831 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Vdd.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vdd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vdd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 216 214 252 230
1 2 0 "s" 0 0 0 64 0 0  216 214
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Vdd
2 833
"Text70"
""
1 422 212 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
832 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Idd.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Idd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Idd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 424 214 460 230
1 2 0 "s" 0 0 0 64 0 0  424 214
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Idd
2 834
"Text75"
""
1 266 212 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
833 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchVCSV.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchVCSV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchVCSV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 268 214 304 230
1 2 0 "s" 0 0 0 64 0 0  268 214
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVchVCSV
2 835
"Text79"
""
1 318 212 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
834 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchPINV.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchPINV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchPINV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 320 214 356 230
1 2 0 "s" 0 0 0 64 0 0  320 214
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVchPINV
2 836
"Text80"
""
1 474 212 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
835 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 476 214 512 230
1 2 0 "s" 0 0 0 64 0 0  476 214
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 MOch_Tm0
2 837
"Text81"
""
1 526 212 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
836 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 528 214 564 230
1 2 0 "s" 0 0 0 64 0 0  528 214
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 MOch_Tm1
2 838
"Text82"
""
1 713 212 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
837 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchCurr.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchCurr.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchCurr.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 715 214 781 230
1 2 0 "s" 0 0 0 64 0 0  715 214
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 HVchCurr
2 839
"Text83"
""
1 583 211 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
838 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 585 213 609 230
1 2 0 "s" 0 0 0 64 0 0  585 213
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 HVchStat
2 840
"Text84"
""
1 623 193 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
839 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 625 213 647 230
1 2 0 "s" 0 0 0 64 0 0  625 213
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 HVchStat
2 841
"Text85"
""
1 661 212 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
840 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchVolt.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchVolt.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchVolt.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 663 214 699 230
1 2 0 "s" 0 0 0 64 0 0  663 214
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 HVchVolt
2 843
"Text86"
""
1 162 242 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
842 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_05:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_05:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Vcc.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vcc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_05:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vcc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 164 244 200 260
1 2 0 "s" 0 0 0 64 0 0  164 244
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Vcc
2 844
"Text87"
""
1 82 241 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
843 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 84 243 108 260
1 2 0 "s" 0 0 0 64 0 0  84 243
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 LVchStat
2 845
"Text88"
""
1 122 241 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
844 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 124 243 148 260
1 2 0 "s" 0 0 0 64 0 0  124 243
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 LVchStat
2 846
"Text89"
""
1 370 242 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
845 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Icc.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Icc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Icc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 372 244 408 260
1 2 0 "s" 0 0 0 64 0 0  372 244
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Icc
2 847
"Text90"
""
1 214 242 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
846 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Vdd.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vdd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vdd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 216 244 252 260
1 2 0 "s" 0 0 0 64 0 0  216 244
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Vdd
2 848
"Text91"
""
1 422 242 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
847 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Idd.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Idd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Idd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 424 244 460 260
1 2 0 "s" 0 0 0 64 0 0  424 244
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Idd
2 849
"Text92"
""
1 266 242 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
848 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchVCSV.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchVCSV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchVCSV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 268 244 304 260
1 2 0 "s" 0 0 0 64 0 0  268 244
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVchVCSV
2 850
"Text93"
""
1 318 242 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
849 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchPINV.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchPINV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchPINV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 320 244 356 260
1 2 0 "s" 0 0 0 64 0 0  320 244
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVchPINV
2 851
"Text94"
""
1 474 242 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
850 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 476 244 512 260
1 2 0 "s" 0 0 0 64 0 0  476 244
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 MOch_Tm0
2 852
"Text95"
""
1 526 242 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
851 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 528 244 564 260
1 2 0 "s" 0 0 0 64 0 0  528 244
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 MOch_Tm1
2 853
"Text96"
""
1 713 242 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
852 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchCurr.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchCurr.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchCurr.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 715 244 781 260
1 2 0 "s" 0 0 0 64 0 0  715 244
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 HVchCurr
2 854
"Text100"
""
1 583 241 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
853 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 585 243 609 260
1 2 0 "s" 0 0 0 64 0 0  585 243
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 HVchStat
2 855
"Text101"
""
1 623 223 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
854 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 625 243 647 260
1 2 0 "s" 0 0 0 64 0 0  625 243
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 HVchStat
2 856
"Text102"
""
1 661 242 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
855 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchVolt.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchVolt.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchVolt.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 663 244 699 260
1 2 0 "s" 0 0 0 64 0 0  663 244
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 HVchVolt
2 858
"Text103"
""
1 162 272 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
857 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_06:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_06:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Vcc.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vcc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_06:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vcc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 164 274 200 290
1 2 0 "s" 0 0 0 64 0 0  164 274
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Vcc
2 859
"Text104"
""
1 82 271 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
858 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 84 273 108 290
1 2 0 "s" 0 0 0 64 0 0  84 273
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 LVchStat
2 860
"Text105"
""
1 122 271 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
859 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 124 273 148 290
1 2 0 "s" 0 0 0 64 0 0  124 273
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 LVchStat
2 861
"Text106"
""
1 370 272 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
860 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Icc.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Icc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Icc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 372 274 408 290
1 2 0 "s" 0 0 0 64 0 0  372 274
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Icc
2 862
"Text107"
""
1 214 272 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
861 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Vdd.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vdd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vdd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 216 274 252 290
1 2 0 "s" 0 0 0 64 0 0  216 274
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Vdd
2 863
"Text108"
""
1 422 272 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
862 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Idd.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Idd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Idd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 424 274 460 290
1 2 0 "s" 0 0 0 64 0 0  424 274
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Idd
2 864
"Text109"
""
1 266 272 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
863 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchVCSV.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchVCSV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchVCSV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 268 274 304 290
1 2 0 "s" 0 0 0 64 0 0  268 274
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVchVCSV
2 865
"Text110"
""
1 318 272 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
864 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchPINV.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchPINV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchPINV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 320 274 356 290
1 2 0 "s" 0 0 0 64 0 0  320 274
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVchPINV
2 866
"Text111"
""
1 474 272 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
865 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 476 274 512 290
1 2 0 "s" 0 0 0 64 0 0  476 274
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 MOch_Tm0
2 867
"Text112"
""
1 526 272 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
866 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 528 274 564 290
1 2 0 "s" 0 0 0 64 0 0  528 274
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 MOch_Tm1
2 868
"Text113"
""
1 713 272 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
867 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchCurr.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchCurr.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchCurr.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 715 274 781 290
1 2 0 "s" 0 0 0 64 0 0  715 274
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 HVchCurr
2 869
"Text114"
""
1 583 271 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
868 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 585 273 609 290
1 2 0 "s" 0 0 0 64 0 0  585 273
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 HVchStat
2 870
"Text115"
""
1 623 253 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
869 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 625 273 647 290
1 2 0 "s" 0 0 0 64 0 0  625 273
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 HVchStat
2 871
"Text116"
""
1 661 272 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
870 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchVolt.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchVolt.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchVolt.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 663 274 699 290
1 2 0 "s" 0 0 0 64 0 0  663 274
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 HVchVolt
2 873
"Text117"
""
1 162 302 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
872 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_07:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_07:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Vcc.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vcc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_07:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vcc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 164 304 200 320
1 2 0 "s" 0 0 0 64 0 0  164 304
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Vcc
2 874
"Text118"
""
1 82 301 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
873 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 84 303 108 320
1 2 0 "s" 0 0 0 64 0 0  84 303
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 LVchStat
2 875
"Text119"
""
1 122 301 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
874 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 124 303 148 320
1 2 0 "s" 0 0 0 64 0 0  124 303
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 LVchStat
2 876
"Text120"
""
1 370 302 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
875 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Icc.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Icc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Icc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 372 304 408 320
1 2 0 "s" 0 0 0 64 0 0  372 304
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Icc
2 877
"Text121"
""
1 214 302 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
876 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Vdd.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vdd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vdd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 216 304 252 320
1 2 0 "s" 0 0 0 64 0 0  216 304
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Vdd
2 878
"Text122"
""
1 422 302 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
877 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Idd.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Idd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Idd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 424 304 460 320
1 2 0 "s" 0 0 0 64 0 0  424 304
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Idd
2 879
"Text123"
""
1 266 302 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
878 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchVCSV.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchVCSV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchVCSV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 268 304 304 320
1 2 0 "s" 0 0 0 64 0 0  268 304
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVchVCSV
2 880
"Text124"
""
1 318 302 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
879 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchPINV.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchPINV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchPINV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 320 304 356 320
1 2 0 "s" 0 0 0 64 0 0  320 304
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVchPINV
2 881
"Text125"
""
1 474 302 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
880 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 476 304 512 320
1 2 0 "s" 0 0 0 64 0 0  476 304
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 MOch_Tm0
2 882
"Text126"
""
1 526 302 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
881 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 528 304 564 320
1 2 0 "s" 0 0 0 64 0 0  528 304
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 MOch_Tm1
2 883
"Text127"
""
1 713 302 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
882 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchCurr.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchCurr.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchCurr.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 715 304 781 320
1 2 0 "s" 0 0 0 64 0 0  715 304
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 HVchCurr
2 884
"Text128"
""
1 583 301 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
883 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 585 303 609 320
1 2 0 "s" 0 0 0 64 0 0  585 303
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 HVchStat
2 885
"Text129"
""
1 623 283 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
884 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 625 303 647 320
1 2 0 "s" 0 0 0 64 0 0  625 303
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 HVchStat
2 886
"Text130"
""
1 661 302 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
885 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchVolt.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchVolt.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchVolt.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 663 304 699 320
1 2 0 "s" 0 0 0 64 0 0  663 304
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 HVchVolt
2 888
"Text131"
""
1 162 332 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
887 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_08:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_08:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Vcc.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vcc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_08:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vcc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 164 334 200 350
1 2 0 "s" 0 0 0 64 0 0  164 334
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Vcc
2 889
"Text132"
""
1 82 331 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
888 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 84 333 108 350
1 2 0 "s" 0 0 0 64 0 0  84 333
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 LVchStat
2 890
"Text133"
""
1 122 331 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
889 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 124 333 148 350
1 2 0 "s" 0 0 0 64 0 0  124 333
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 LVchStat
2 891
"Text134"
""
1 370 332 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
890 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Icc.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Icc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Icc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 372 334 408 350
1 2 0 "s" 0 0 0 64 0 0  372 334
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Icc
2 892
"Text135"
""
1 214 332 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
891 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Vdd.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vdd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vdd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 216 334 252 350
1 2 0 "s" 0 0 0 64 0 0  216 334
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Vdd
2 893
"Text136"
""
1 422 332 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
892 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Idd.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Idd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Idd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 424 334 460 350
1 2 0 "s" 0 0 0 64 0 0  424 334
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Idd
2 894
"Text137"
""
1 266 332 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
893 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchVCSV.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchVCSV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchVCSV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 268 334 304 350
1 2 0 "s" 0 0 0 64 0 0  268 334
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVchVCSV
2 895
"Text138"
""
1 318 332 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
894 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchPINV.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchPINV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchPINV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 320 334 356 350
1 2 0 "s" 0 0 0 64 0 0  320 334
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVchPINV
2 896
"Text139"
""
1 474 332 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
895 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 476 334 512 350
1 2 0 "s" 0 0 0 64 0 0  476 334
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 MOch_Tm0
2 897
"Text140"
""
1 526 332 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
896 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 528 334 564 350
1 2 0 "s" 0 0 0 64 0 0  528 334
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 MOch_Tm1
2 898
"Text141"
""
1 713 332 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
897 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchCurr.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchCurr.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchCurr.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 715 334 781 350
1 2 0 "s" 0 0 0 64 0 0  715 334
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 HVchCurr
2 899
"Text142"
""
1 583 331 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
898 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 585 333 609 350
1 2 0 "s" 0 0 0 64 0 0  585 333
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 HVchStat
2 900
"Text143"
""
1 623 313 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
899 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 625 333 647 350
1 2 0 "s" 0 0 0 64 0 0  625 333
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 HVchStat
2 901
"Text144"
""
1 661 332 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
900 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchVolt.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchVolt.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchVolt.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 663 334 699 350
1 2 0 "s" 0 0 0 64 0 0  663 334
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 HVchVolt
2 903
"Text145"
""
1 162 362 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
902 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_09:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_09:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Vcc.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vcc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_09:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vcc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 164 364 200 380
1 2 0 "s" 0 0 0 64 0 0  164 364
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Vcc
2 904
"Text146"
""
1 82 361 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
903 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 84 363 108 380
1 2 0 "s" 0 0 0 64 0 0  84 363
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 LVchStat
2 905
"Text147"
""
1 122 361 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
904 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 124 363 148 380
1 2 0 "s" 0 0 0 64 0 0  124 363
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 LVchStat
2 906
"Text148"
""
1 370 362 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
905 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Icc.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Icc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Icc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 372 364 408 380
1 2 0 "s" 0 0 0 64 0 0  372 364
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Icc
2 907
"Text149"
""
1 214 362 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
906 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Vdd.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vdd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vdd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 216 364 252 380
1 2 0 "s" 0 0 0 64 0 0  216 364
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Vdd
2 908
"Text150"
""
1 422 362 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
907 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Idd.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Idd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Idd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 424 364 460 380
1 2 0 "s" 0 0 0 64 0 0  424 364
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Idd
2 909
"Text151"
""
1 266 362 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
908 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchVCSV.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchVCSV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchVCSV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 268 364 304 380
1 2 0 "s" 0 0 0 64 0 0  268 364
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVchVCSV
2 910
"Text152"
""
1 318 362 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
909 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchPINV.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchPINV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchPINV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 320 364 356 380
1 2 0 "s" 0 0 0 64 0 0  320 364
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVchPINV
2 911
"Text153"
""
1 474 362 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
910 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 476 364 512 380
1 2 0 "s" 0 0 0 64 0 0  476 364
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 MOch_Tm0
2 912
"Text154"
""
1 526 362 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
911 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 528 364 564 380
1 2 0 "s" 0 0 0 64 0 0  528 364
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 MOch_Tm1
2 913
"Text155"
""
1 713 362 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
912 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchCurr.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchCurr.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchCurr.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 715 364 781 380
1 2 0 "s" 0 0 0 64 0 0  715 364
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 HVchCurr
2 914
"Text156"
""
1 583 361 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
913 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 585 363 609 380
1 2 0 "s" 0 0 0 64 0 0  585 363
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 HVchStat
2 915
"Text157"
""
1 623 343 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
914 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 625 363 647 380
1 2 0 "s" 0 0 0 64 0 0  625 363
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 HVchStat
2 916
"Text158"
""
1 661 362 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
915 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchVolt.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchVolt.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchVolt.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 663 364 699 380
1 2 0 "s" 0 0 0 64 0 0  663 364
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 HVchVolt
2 918
"Text159"
""
1 162 392 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
917 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_10:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_10:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Vcc.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vcc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_10:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vcc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 164 394 200 410
1 2 0 "s" 0 0 0 64 0 0  164 394
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Vcc
2 919
"Text160"
""
1 82 391 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
918 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 84 393 108 410
1 2 0 "s" 0 0 0 64 0 0  84 393
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 LVchStat
2 920
"Text161"
""
1 122 391 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
919 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 124 393 148 410
1 2 0 "s" 0 0 0 64 0 0  124 393
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 LVchStat
2 921
"Text162"
""
1 370 392 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
920 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Icc.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Icc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Icc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 372 394 408 410
1 2 0 "s" 0 0 0 64 0 0  372 394
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Icc
2 922
"Text163"
""
1 214 392 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
921 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Vdd.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vdd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vdd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 216 394 252 410
1 2 0 "s" 0 0 0 64 0 0  216 394
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Vdd
2 923
"Text164"
""
1 422 392 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
922 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Idd.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Idd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Idd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 424 394 460 410
1 2 0 "s" 0 0 0 64 0 0  424 394
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Idd
2 924
"Text165"
""
1 266 392 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
923 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchVCSV.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchVCSV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchVCSV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 268 394 304 410
1 2 0 "s" 0 0 0 64 0 0  268 394
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVchVCSV
2 925
"Text166"
""
1 318 392 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
924 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchPINV.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchPINV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchPINV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 320 394 356 410
1 2 0 "s" 0 0 0 64 0 0  320 394
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVchPINV
2 926
"Text167"
""
1 474 392 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
925 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 476 394 512 410
1 2 0 "s" 0 0 0 64 0 0  476 394
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 MOch_Tm0
2 927
"Text168"
""
1 526 392 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
926 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 528 394 564 410
1 2 0 "s" 0 0 0 64 0 0  528 394
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 MOch_Tm1
2 928
"Text169"
""
1 713 392 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
927 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchCurr.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchCurr.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchCurr.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 715 394 781 410
1 2 0 "s" 0 0 0 64 0 0  715 394
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 HVchCurr
2 929
"Text170"
""
1 583 391 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
928 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 585 393 609 410
1 2 0 "s" 0 0 0 64 0 0  585 393
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 HVchStat
2 930
"Text171"
""
1 623 373 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
929 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 625 393 647 410
1 2 0 "s" 0 0 0 64 0 0  625 393
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 HVchStat
2 931
"Text172"
""
1 661 392 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
930 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchVolt.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchVolt.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchVolt.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 663 394 699 410
1 2 0 "s" 0 0 0 64 0 0  663 394
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 HVchVolt
2 933
"Text173"
""
1 162 422 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
932 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Vcc.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vcc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vcc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 164 424 200 440
1 2 0 "s" 0 0 0 64 0 0  164 424
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Vcc
2 934
"Text174"
""
1 82 421 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
933 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 84 423 108 440
1 2 0 "s" 0 0 0 64 0 0  84 423
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 LVchStat
2 935
"Text175"
""
1 122 421 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
934 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 124 423 148 440
1 2 0 "s" 0 0 0 64 0 0  124 423
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 LVchStat
2 936
"Text176"
""
1 370 422 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
935 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Icc.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Icc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Icc.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 372 424 408 440
1 2 0 "s" 0 0 0 64 0 0  372 424
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Icc
2 937
"Text177"
""
1 214 422 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
936 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Vdd.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vdd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Vdd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 216 424 252 440
1 2 0 "s" 0 0 0 64 0 0  216 424
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Vdd
2 938
"Text178"
""
1 422 422 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
937 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVch_Idd.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Idd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVch_Idd.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 424 424 460 440
1 2 0 "s" 0 0 0 64 0 0  424 424
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVch_Idd
2 939
"Text179"
""
1 266 422 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
938 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchVCSV.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchVCSV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchVCSV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 268 424 304 440
1 2 0 "s" 0 0 0 64 0 0  268 424
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVchVCSV
2 940
"Text180"
""
1 318 422 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
939 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.LVchPINV.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.LVchPINV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.LVchPINV.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 320 424 356 440
1 2 0 "s" 0 0 0 64 0 0  320 424
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 LVchPINV
2 941
"Text181"
""
1 474 422 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
940 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 476 424 512 440
1 2 0 "s" 0 0 0 64 0 0  476 424
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 MOch_Tm0
2 942
"Text182"
""
1 526 422 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
941 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.MOch_Tm0.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 528 424 564 440
1 2 0 "s" 0 0 0 64 0 0  528 424
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 MOch_Tm1
2 943
"Text183"
""
1 713 422 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
942 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchCurr.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchCurr.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchCurr.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 715 424 781 440
1 2 0 "s" 0 0 0 64 0 0  715 424
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 HVchCurr
2 944
"Text184"
""
1 583 421 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
943 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 585 423 609 440
1 2 0 "s" 0 0 0 64 0 0  585 423
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 HVchStat
2 945
"Text185"
""
1 623 403 E E E 1 E 1 E N {0,0,0} E N {204,204,204} E E
 E E
944 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchStat.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 625 423 647 440
1 2 0 "s" 0 0 0 64 0 0  625 423
 1
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
1
LANG:1 8 HVchStat
2 946
"Text186"
""
1 661 422 E E E 1 E 1 E N {0,0,0} E N {236,233,216} E E
 E E
945 0 0 0 0 0
EE E
0
1
LANG:1 0 
1
"dashclr"N "_Transparent"
"main()
{
  EP_textFieldIn();
  
}

EP_textFieldIn()
{
dyn_errClass err;
string datapoint,dp1;
int channelnb,i, iLimit;
int crate,count;
string channel,dplimit;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);
dpGet(\"SCTmops1:Limit.Indx:_online.._value\", iLimit);

//Connect the channelnumber
channel = \"SCTmops1:Sector.Row_00.ST_11:_online.._value\";
sprintf(datapoint, \"Crate%02d.Channel%02d.HVchVolt.Recv:_online.._value\",crate, channelnb);
dplimit = \"SCTmops1:Limit.Indx:_online.._value\";

dpConnect(\"EP_textFieldInCB\", channel);
dpConnect(\"EP_textFieldInCB1\", datapoint);
dpConnect(\"EP_textFieldInCB2\", dplimit);
                 
}


EP_textFieldInCB(string dp, float channelnb)
{ 
int crate;
float temperature;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
 
   sprintf(dp1, \"Crate%02d.Channel%02d.HVchVolt.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);
   //DebugN(\"channel\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}



EP_textFieldInCB1(string dp, float temperature)
{ 
int crate;
string dp1,sTmp;

EP_setBackColorE(dp,temperature);
//DebugN(\"temperature\", dp1, temperature);

//sprintf(sTmp,\"%f\",temperature);
setValue(\"\", \"text\", temperature );

}

EP_textFieldInCB2(string dp, float limit)
{ 
int crate;
int temperature, channelnb;
string dp1,sTmp;

dpGet(\"Crate.Numb:_original.._value\", crate);
dpGet(\"SCTmops1:Sector.Row_00.ST_11:_online.._value\", channelnb);

   sprintf(dp1, \"Crate%02d.Channel%02d.HVchVolt.Recv:_online.._value\",crate, channelnb);
   dpGet(dp1,temperature);
   EP_setBackColorE(dp1,temperature);

//DebugN(\"dplimit\", dp1, temperature);


}" 0
 E 0 1 1 0 1 E U  1 E 663 424 699 440
1 2 0 "s" 0 0 0 64 0 0  663 424
 1
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
1
LANG:1 8 HVchVolt
21 267
"SpinButton49"
""
1 120 630 E E E 1 E 1 E N "_WindowText" E N "_Window" E E
 E E
266 0 0 0 0 0
EE E
0
1
LANG:1 0 
0
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
118 628 192 654
0
"// SimpleCtrlScriptStart {invalid}
main()
{
  EP_textFieldIn();
  EP_setInvalid();
}

EP_textFieldIn()
{
dyn_errClass err;

  if( dpSubStr( \"SCTmops1:Limit.Indx\", DPSUB_DP_EL ) == \"\" )
  {
    setValue(\"\", \"color\", \"_dpdoesnotexist\");
    return;
  }

  dpConnect(\"EP_textFieldInCB\",
            \"SCTmops1:Limit.Indx:_online.._value\");
  err = getLastError();
  if (dynlen(err) > 0)
    setValue(\"\", \"color\", \"_dpdoesnotexist\");

}


EP_textFieldInCB(string dp, int iNewValue)
{
  setValue(\"\", \"text\", iNewValue);
}

EP_setInvalid()
{
dyn_errClass err;

  if( dpSubStr( \"SCTmops1:Limit.Indx:_online.._invalid\", DPSUB_DP_EL ) == \"\" )
  {
    setValue(\"\", \"color\", \"_dpdoesnotexist\");
    return;
  }

  dpConnect(\"EP_setInvalidCB\",
            \"SCTmops1:Limit.Indx:_online.._invalid\");
  err = getLastError();
  if (dynlen(err) > 0)
    setValue(\"\", \"color\", \"_dpdoesnotexist\");

}

EP_setInvalidCB(string dp, bool boInvalid)
{
  setValue(\"\", \"color\", (boInvalid ? \"_invalid\" : \"\"));
}

// SimpleCtrlScript {EP_textFieldIn}
// DP {SCTmops1:Sector.Row_00.ST_01}
// DPConfig {:_online.._value}
// DPType {int}
// UseDPUnit {FALSE}
// UseDPFormat {FALSE}
// SimpleCtrlScriptEnd {EP_textFieldIn}
// SimpleCtrlScript {EP_setInvalid}
// DP {SCTmops1:Sector.Row_00.ST_01}
// DPConfig {:_online.._invalid}
// DPType {bool}
// Attribut {color}
// SimpleCtrlScriptEnd {EP_setInvalid}
" 0

"// SimpleCtrlScriptStart {invalid}
main()
{
  EP_textFieldOut();
}

EP_textFieldOut()
{
int iNewValue;
dyn_errClass err;
string sTmp;
string sFormat, sDp;

  getValue(\"\", \"text\", sTmp);
  sscanf(sTmp, \"%d\", iNewValue);

  sDp = dpSubStr(\"SCTmops1:Limit.Indx:_original.._value\",  DPSUB_SYS_DP_EL);
  if ( strpos(sDp,\".\") < 1 )
    sDp += \".\";

  sFormat = dpGetFormat( sDp );
  if( !checkStringFormat(sTmp, sFormat) )
  {
    ChildPanelOnCentral( \"vision/MessageWarning\",
                         getCatStr( \"e_para\", \"warning\" ),
                         makeDynString( getCatStr( \"e_para\", \"wrongFormat\" )));
    return;
  }

  dpSetWait(\"SCTmops1:Limit.Indx:_original.._value\", sTmp);
  err = getLastError();
  if (dynlen(err) > 0)
    errorDialog(err);
}

// SimpleCtrlScript {EP_textFieldOut}
// DP {SCTmops1:Sector.Row_00.ST_00}
// Config {:_original.._value}
// DPType {int}
// SimpleCtrlScriptEnd {EP_textFieldOut}
" 0

E

N 0 100 1 0 0 1
13 596
"Button1"
""
1 20 50 E E E 1 E 1 E N "_3DText" E N {204,204,204} E E
 E E
595 0 0 0 0 0
EE E
0
1
LANG:1 0 
0
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-120-100-100-*-*-iso8859-1|-13,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
18 48 42 72
T 
1
LANG:1 1 !
"// SimpleCtrlScriptStart {valid}
main()
{
  EP_childPanelOn();
}

EP_childPanelOn()
{
  ChildPanelOnCentral(\"subpanels/BinStat.pnl\",
      \"\",
      makeDynString(\"\"));
}

// SimpleCtrlScript {EP_childPanelOn}
// Function {ChildPanelOnCentral}
// File {subpanels/BinStat.pnl}
// Panel {}
// Parent {}
// Module {}
// OffsetX {0}
// OffsetY {0}
// SimpleCtrlScriptEnd {EP_childPanelOn}
" 0
 E E E
13 613
"StatExplHV"
""
1 40 50 E E E 1 E 1 E N "_3DText" E N {204,204,204} E E
 E E
612 0 0 0 0 0
EE E
0
1
LANG:1 0 
0
1
LANG:1 105 -microsoft windows-Arial-bold-r-normal-*-*-120-100-100-*-*-iso8859-1|-13,0,0,0,700,0,0,0,0,3,2,1,34,Arial
0 ""
38 48 62 72
T 
1
LANG:1 1 !
"// SimpleCtrlScriptStart {invalid}
main()
{
  EP_childPanelOn();
}

EP_childPanelOn()
{
  ChildPanelOnCentral(\"subpanels/BinStatHV.pnl\",
      \"\",
      makeDynString(\"\"));
}

// SimpleCtrlScript {EP_childPanelOn}
// Function {ChildPanelOnCentral}
// File {subpanels/BinStat.pnl}
// Panel {}
// Parent {}
// Module {}
// OffsetX {0}
// OffsetY {0}
// SimpleCtrlScriptEnd {EP_childPanelOn}
" 0
 E E E
14 781
"TextField3"
""
1 230 670 E E E 1 E 1 E N "_WindowText" E N "_Window" E E
 E E
780 0 0 0 0 0
EE E
0
1
LANG:1 0 
0
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
228 668 282 694
3 "s" 0 0 0 0 0 0 
E
"main()
{
  EP_textFieldIn();
  EP_setInvalid();
}

EP_textFieldIn()
{
dyn_errClass err;

  if( dpSubStr( \"SCTmops1:Limit.Indx\", DPSUB_DP_EL ) == \"\" )
  {
    setValue(\"\", \"color\", \"_dpdoesnotexist\");
    return;
  }

  dpConnect(\"EP_textFieldInCB\",
            \"SCTmops1:Limit.Indx:_online.._value\");
  err = getLastError();
  if (dynlen(err) > 0)
    setValue(\"\", \"color\", \"_dpdoesnotexist\");

}


EP_textFieldInCB(string dp, int iNewValue)
{
  setValue(\"\", \"text\", iNewValue);
}

EP_setInvalid()
{
dyn_errClass err;

  if( dpSubStr( \"SCTmops1:Limit.Indx:_online.._invalid\", DPSUB_DP_EL ) == \"\" )
  {
    setValue(\"\", \"color\", \"_dpdoesnotexist\");
    return;
  }

  dpConnect(\"EP_setInvalidCB\",
            \"SCTmops1:Limit.Indx:_online.._invalid\");
  err = getLastError();
  if (dynlen(err) > 0)
    setValue(\"\", \"color\", \"_dpdoesnotexist\");

}

EP_setInvalidCB(string dp, bool boInvalid)
{
  setValue(\"\", \"color\", (boInvalid ? \"_invalid\" : \"\"));
}
" 0

"// SimpleCtrlScriptStart {invalid}
main()
{
  EP_textFieldOut();
}

EP_textFieldOut()
{
int iNewValue;
dyn_errClass err;
string sTmp;
string sFormat, sDp;

  getValue(\"\", \"text\", sTmp);
  sscanf(sTmp, \"%d\", iNewValue);

  sDp = dpSubStr(\"SCTmops1:Limit.Indx:_original.._value\",  DPSUB_SYS_DP_EL);
  if ( strpos(sDp,\".\") < 1 )
    sDp += \".\";

  sFormat = dpGetFormat( sDp );
  if( !checkStringFormat(sTmp, sFormat) )
  {
    ChildPanelOnCentral( \"vision/MessageWarning\",
                         getCatStr( \"e_para\", \"warning\" ),
                         makeDynString( getCatStr( \"e_para\", \"wrongFormat\" )));
    return;
  }

  dpSetWait(\"SCTmops1:Limit.Indx:_original.._value\", sTmp);
  err = getLastError();
  if (dynlen(err) > 0)
    errorDialog(err);
}

// SimpleCtrlScript {EP_textFieldOut}
// DP {HVch.Numb}
// Config {:_original.._value}
// DPType {int}
// SimpleCtrlScriptEnd {EP_textFieldOut}
" 0

21 960
"SpinButton1"
""
1 30 184 E E E 1 E 1 E N "_WindowText" E N "_Window" E E
 E E
959 0 0 0 0 0
EE E
0
1
LANG:1 0 
0
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
28 182 72 208
0
"// SimpleCtrlScriptStart {invalid}
main()
{
  EP_textFieldIn();
  EP_setInvalid();
}

EP_textFieldIn()
{
dyn_errClass err;

  if( dpSubStr( \"SCTmops1:Sector.Row_00.ST_03:_online.._value\", DPSUB_DP_EL ) == \"\" )
  {
    setValue(\"\", \"color\", \"_dpdoesnotexist\");
    return;
  }

  dpConnect(\"EP_textFieldInCB\",
            \"SCTmops1:Sector.Row_00.ST_03:_online.._value\");
  err = getLastError();
  if (dynlen(err) > 0)
    setValue(\"\", \"color\", \"_dpdoesnotexist\");

}

EP_textFieldInCB(string dp, int iNewValue)
{
  setValue(\"\", \"text\", dpValToString(dp, iNewValue, TRUE) );
}

EP_setInvalid()
{
dyn_errClass err;

  if( dpSubStr( \"SCTmops1:Sector.Row_00.ST_03:_online.._invalid\", DPSUB_DP_EL ) == \"\" )
  {
    setValue(\"\", \"color\", \"_dpdoesnotexist\");
    return;
  }

  dpConnect(\"EP_setInvalidCB\",
            \"SCTmops1:Sector.Row_00.ST_03:_online.._invalid\");
  err = getLastError();
  if (dynlen(err) > 0)
    setValue(\"\", \"color\", \"_dpdoesnotexist\");

}

EP_setInvalidCB(string dp, bool boInvalid)
{
  setValue(\"\", \"color\", (boInvalid ? \"_invalid\" : \"\"));
}

// SimpleCtrlScript {EP_textFieldIn}
// DP {SCTmops1:Sector.Row_00.ST_03}
// DPConfig {:_online.._value}
// DPType {int}
// UseDPUnit {TRUE}
// UseDPFormat {TRUE}
// SimpleCtrlScriptEnd {EP_textFieldIn}
// SimpleCtrlScript {EP_setInvalid}
// DP {SCTmops1:Sector.Row_00.ST_04}
// DPConfig {:_online.._invalid}
// DPType {bool}
// Attribut {color}
// SimpleCtrlScriptEnd {EP_setInvalid}
" 0

"// SimpleCtrlScriptStart {invalid}
main()
{
  EP_textFieldOut();
}

EP_textFieldOut()
{
int iNewValue;
dyn_errClass err;
string sTmp;
string sFormat, sDp;

  getValue(\"\", \"text\", sTmp);
  sscanf(sTmp, \"%d\", iNewValue);

  sDp = dpSubStr(\"SCTmops1:Sector.Row_00.ST_03:_original.._value\",  DPSUB_SYS_DP_EL);
  if ( strpos(sDp,\".\") < 1 )
    sDp += \".\";

  sFormat = dpGetFormat( sDp );
  if( !checkStringFormat(sTmp, sFormat) )
  {
    ChildPanelOnCentral( \"vision/MessageWarning\",
                         getCatStr( \"e_para\", \"warning\" ),
                         makeDynString( getCatStr( \"e_para\", \"wrongFormat\" )));
    return;
  }

  dpSetWait(\"SCTmops1:Sector.Row_00.ST_03:_original.._value\", sTmp);
  err = getLastError();
  if (dynlen(err) > 0)
    errorDialog(err);
}

// SimpleCtrlScript {EP_textFieldOut}
// DP {SCTmops1:Sector.Row_00.ST_00}
// Config {:_original.._value}
// DPType {int}
// SimpleCtrlScriptEnd {EP_textFieldOut}
" 0

E

N 0 100 1 0 0 1
21 961
"SpinButton5"
""
1 30 213 E E E 1 E 1 E N "_WindowText" E N "_Window" E E
 E E
960 0 0 0 0 0
EE E
0
1
LANG:1 0 
0
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
28 211 72 237
0
"// SimpleCtrlScriptStart {valid}
main()
{
  EP_textFieldIn();
  EP_setInvalid();
}

EP_textFieldIn()
{
dyn_errClass err;

  if( dpSubStr( \"SCTmops1:Sector.Row_00.ST_04:_online.._value\", DPSUB_DP_EL ) == \"\" )
  {
    setValue(\"\", \"color\", \"_dpdoesnotexist\");
    return;
  }

  dpConnect(\"EP_textFieldInCB\",
            \"SCTmops1:Sector.Row_00.ST_04:_online.._value\");
  err = getLastError();
  if (dynlen(err) > 0)
    setValue(\"\", \"color\", \"_dpdoesnotexist\");

}


EP_textFieldInCB(string dp, int iNewValue)
{
  setValue(\"\", \"text\", iNewValue);
}

EP_setInvalid()
{
dyn_errClass err;

  if( dpSubStr( \"SCTmops1:Sector.Row_00.ST_04:_online.._invalid\", DPSUB_DP_EL ) == \"\" )
  {
    setValue(\"\", \"color\", \"_dpdoesnotexist\");
    return;
  }

  dpConnect(\"EP_setInvalidCB\",
            \"SCTmops1:Sector.Row_00.ST_04:_online.._invalid\");
  err = getLastError();
  if (dynlen(err) > 0)
    setValue(\"\", \"color\", \"_dpdoesnotexist\");

}

EP_setInvalidCB(string dp, bool boInvalid)
{
  setValue(\"\", \"color\", (boInvalid ? \"_invalid\" : \"\"));
}

// SimpleCtrlScript {EP_textFieldIn}
// DP {SCTmops1:Sector.Row_00.ST_04}
// DPConfig {:_online.._value}
// DPType {int}
// UseDPUnit {FALSE}
// UseDPFormat {FALSE}
// SimpleCtrlScriptEnd {EP_textFieldIn}
// SimpleCtrlScript {EP_setInvalid}
// DP {SCTmops1:Sector.Row_00.ST_04}
// DPConfig {:_online.._invalid}
// DPType {bool}
// Attribut {color}
// SimpleCtrlScriptEnd {EP_setInvalid}
" 0

"// SimpleCtrlScriptStart {invalid}
main()
{
  EP_textFieldOut();
}

EP_textFieldOut()
{
int iNewValue;
dyn_errClass err;
string sTmp;
string sFormat, sDp;

  getValue(\"\", \"text\", sTmp);
  sscanf(sTmp, \"%d\", iNewValue);

  sDp = dpSubStr(\"SCTmops1:Sector.Row_00.ST_04:_original.._value\",  DPSUB_SYS_DP_EL);
  if ( strpos(sDp,\".\") < 1 )
    sDp += \".\";

  sFormat = dpGetFormat( sDp );
  if( !checkStringFormat(sTmp, sFormat) )
  {
    ChildPanelOnCentral( \"vision/MessageWarning\",
                         getCatStr( \"e_para\", \"warning\" ),
                         makeDynString( getCatStr( \"e_para\", \"wrongFormat\" )));
    return;
  }

  dpSetWait(\"SCTmops1:Sector.Row_00.ST_04:_original.._value\", sTmp);
  err = getLastError();
  if (dynlen(err) > 0)
    errorDialog(err);
}

// SimpleCtrlScript {EP_textFieldOut}
// DP {SCTmops1:Sector.Row_00.ST_00}
// Config {:_original.._value}
// DPType {int}
// SimpleCtrlScriptEnd {EP_textFieldOut}
" 0

E

N 0 100 1 0 0 1
21 962
"SpinButton6"
""
1 30 242 E E E 1 E 1 E N "_WindowText" E N "_Window" E E
 E E
961 0 0 0 0 0
EE E
0
1
LANG:1 0 
0
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
28 240 72 266
0
"// SimpleCtrlScriptStart {valid}
main()
{
  EP_textFieldIn();
  EP_setInvalid();
}

EP_textFieldIn()
{
dyn_errClass err;

  if( dpSubStr( \"SCTmops1:Sector.Row_00.ST_05:_online.._value\", DPSUB_DP_EL ) == \"\" )
  {
    setValue(\"\", \"color\", \"_dpdoesnotexist\");
    return;
  }

  dpConnect(\"EP_textFieldInCB\",
            \"SCTmops1:Sector.Row_00.ST_05:_online.._value\");
  err = getLastError();
  if (dynlen(err) > 0)
    setValue(\"\", \"color\", \"_dpdoesnotexist\");

}


EP_textFieldInCB(string dp, int iNewValue)
{
  setValue(\"\", \"text\", iNewValue);
}

EP_setInvalid()
{
dyn_errClass err;

  if( dpSubStr( \"SCTmops1:Sector.Row_00.ST_05:_online.._invalid\", DPSUB_DP_EL ) == \"\" )
  {
    setValue(\"\", \"color\", \"_dpdoesnotexist\");
    return;
  }

  dpConnect(\"EP_setInvalidCB\",
            \"SCTmops1:Sector.Row_00.ST_05:_online.._invalid\");
  err = getLastError();
  if (dynlen(err) > 0)
    setValue(\"\", \"color\", \"_dpdoesnotexist\");

}

EP_setInvalidCB(string dp, bool boInvalid)
{
  setValue(\"\", \"color\", (boInvalid ? \"_invalid\" : \"\"));
}

// SimpleCtrlScript {EP_textFieldIn}
// DP {SCTmops1:Sector.Row_00.ST_05}
// DPConfig {:_online.._value}
// DPType {int}
// UseDPUnit {FALSE}
// UseDPFormat {FALSE}
// SimpleCtrlScriptEnd {EP_textFieldIn}
// SimpleCtrlScript {EP_setInvalid}
// DP {SCTmops1:Sector.Row_00.ST_05}
// DPConfig {:_online.._invalid}
// DPType {bool}
// Attribut {color}
// SimpleCtrlScriptEnd {EP_setInvalid}
" 0

"// SimpleCtrlScriptStart {invalid}
main()
{
  EP_textFieldOut();
}

EP_textFieldOut()
{
int iNewValue;
dyn_errClass err;
string sTmp;
string sFormat, sDp;

  getValue(\"\", \"text\", sTmp);
  sscanf(sTmp, \"%d\", iNewValue);

  sDp = dpSubStr(\"SCTmops1:Sector.Row_00.ST_05:_original.._value\",  DPSUB_SYS_DP_EL);
  if ( strpos(sDp,\".\") < 1 )
    sDp += \".\";

  sFormat = dpGetFormat( sDp );
  if( !checkStringFormat(sTmp, sFormat) )
  {
    ChildPanelOnCentral( \"vision/MessageWarning\",
                         getCatStr( \"e_para\", \"warning\" ),
                         makeDynString( getCatStr( \"e_para\", \"wrongFormat\" )));
    return;
  }

  dpSetWait(\"SCTmops1:Sector.Row_00.ST_05:_original.._value\", sTmp);
  err = getLastError();
  if (dynlen(err) > 0)
    errorDialog(err);
}

// SimpleCtrlScript {EP_textFieldOut}
// DP {SCTmops1:Sector.Row_00.ST_00}
// Config {:_original.._value}
// DPType {int}
// SimpleCtrlScriptEnd {EP_textFieldOut}
" 0

E

N 0 100 1 0 0 1
21 963
"SpinButton7"
""
1 30 271 E E E 1 E 1 E N "_WindowText" E N "_Window" E E
 E E
962 0 0 0 0 0
EE E
0
1
LANG:1 0 
0
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
28 269 72 295
0
"// SimpleCtrlScriptStart {valid}
main()
{
  EP_textFieldIn();
  EP_setInvalid();
}

EP_textFieldIn()
{
dyn_errClass err;

  if( dpSubStr( \"SCTmops1:Sector.Row_00.ST_06:_online.._value\", DPSUB_DP_EL ) == \"\" )
  {
    setValue(\"\", \"color\", \"_dpdoesnotexist\");
    return;
  }

  dpConnect(\"EP_textFieldInCB\",
            \"SCTmops1:Sector.Row_00.ST_06:_online.._value\");
  err = getLastError();
  if (dynlen(err) > 0)
    setValue(\"\", \"color\", \"_dpdoesnotexist\");

}


EP_textFieldInCB(string dp, int iNewValue)
{
  setValue(\"\", \"text\", iNewValue);
}

EP_setInvalid()
{
dyn_errClass err;

  if( dpSubStr( \"SCTmops1:Sector.Row_00.ST_06:_online.._invalid\", DPSUB_DP_EL ) == \"\" )
  {
    setValue(\"\", \"color\", \"_dpdoesnotexist\");
    return;
  }

  dpConnect(\"EP_setInvalidCB\",
            \"SCTmops1:Sector.Row_00.ST_06:_online.._invalid\");
  err = getLastError();
  if (dynlen(err) > 0)
    setValue(\"\", \"color\", \"_dpdoesnotexist\");

}

EP_setInvalidCB(string dp, bool boInvalid)
{
  setValue(\"\", \"color\", (boInvalid ? \"_invalid\" : \"\"));
}

// SimpleCtrlScript {EP_textFieldIn}
// DP {SCTmops1:Sector.Row_00.ST_06}
// DPConfig {:_online.._value}
// DPType {int}
// UseDPUnit {FALSE}
// UseDPFormat {FALSE}
// SimpleCtrlScriptEnd {EP_textFieldIn}
// SimpleCtrlScript {EP_setInvalid}
// DP {SCTmops1:Sector.Row_00.ST_06}
// DPConfig {:_online.._invalid}
// DPType {bool}
// Attribut {color}
// SimpleCtrlScriptEnd {EP_setInvalid}
" 0

"// SimpleCtrlScriptStart {invalid}
main()
{
  EP_textFieldOut();
}

EP_textFieldOut()
{
int iNewValue;
dyn_errClass err;
string sTmp;
string sFormat, sDp;

  getValue(\"\", \"text\", sTmp);
  sscanf(sTmp, \"%d\", iNewValue);

  sDp = dpSubStr(\"SCTmops1:Sector.Row_00.ST_06:_original.._value\",  DPSUB_SYS_DP_EL);
  if ( strpos(sDp,\".\") < 1 )
    sDp += \".\";

  sFormat = dpGetFormat( sDp );
  if( !checkStringFormat(sTmp, sFormat) )
  {
    ChildPanelOnCentral( \"vision/MessageWarning\",
                         getCatStr( \"e_para\", \"warning\" ),
                         makeDynString( getCatStr( \"e_para\", \"wrongFormat\" )));
    return;
  }

  dpSetWait(\"SCTmops1:Sector.Row_00.ST_06:_original.._value\", sTmp);
  err = getLastError();
  if (dynlen(err) > 0)
    errorDialog(err);
}

// SimpleCtrlScript {EP_textFieldOut}
// DP {SCTmops1:Sector.Row_00.ST_00}
// Config {:_original.._value}
// DPType {int}
// SimpleCtrlScriptEnd {EP_textFieldOut}
" 0

E

N 0 100 1 0 0 1
21 964
"SpinButton8"
""
1 30 300 E E E 1 E 1 E N "_WindowText" E N "_Window" E E
 E E
963 0 0 0 0 0
EE E
0
1
LANG:1 0 
0
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
28 298 72 324
0
"// SimpleCtrlScriptStart {valid}
main()
{
  EP_textFieldIn();
  EP_setInvalid();
}

EP_textFieldIn()
{
dyn_errClass err;

  if( dpSubStr( \"SCTmops1:Sector.Row_00.ST_07:_online.._value\", DPSUB_DP_EL ) == \"\" )
  {
    setValue(\"\", \"color\", \"_dpdoesnotexist\");
    return;
  }

  dpConnect(\"EP_textFieldInCB\",
            \"SCTmops1:Sector.Row_00.ST_07:_online.._value\");
  err = getLastError();
  if (dynlen(err) > 0)
    setValue(\"\", \"color\", \"_dpdoesnotexist\");

}


EP_textFieldInCB(string dp, int iNewValue)
{
  setValue(\"\", \"text\", iNewValue);
}

EP_setInvalid()
{
dyn_errClass err;

  if( dpSubStr( \"SCTmops1:Sector.Row_00.ST_07:_online.._invalid\", DPSUB_DP_EL ) == \"\" )
  {
    setValue(\"\", \"color\", \"_dpdoesnotexist\");
    return;
  }

  dpConnect(\"EP_setInvalidCB\",
            \"SCTmops1:Sector.Row_00.ST_07:_online.._invalid\");
  err = getLastError();
  if (dynlen(err) > 0)
    setValue(\"\", \"color\", \"_dpdoesnotexist\");

}

EP_setInvalidCB(string dp, bool boInvalid)
{
  setValue(\"\", \"color\", (boInvalid ? \"_invalid\" : \"\"));
}

// SimpleCtrlScript {EP_textFieldIn}
// DP {SCTmops1:Sector.Row_00.ST_07}
// DPConfig {:_online.._value}
// DPType {int}
// UseDPUnit {FALSE}
// UseDPFormat {FALSE}
// SimpleCtrlScriptEnd {EP_textFieldIn}
// SimpleCtrlScript {EP_setInvalid}
// DP {SCTmops1:Sector.Row_00.ST_07}
// DPConfig {:_online.._invalid}
// DPType {bool}
// Attribut {color}
// SimpleCtrlScriptEnd {EP_setInvalid}
" 0

"// SimpleCtrlScriptStart {invalid}
main()
{
  EP_textFieldOut();
}

EP_textFieldOut()
{
int iNewValue;
dyn_errClass err;
string sTmp;
string sFormat, sDp;

  getValue(\"\", \"text\", sTmp);
  sscanf(sTmp, \"%d\", iNewValue);

  sDp = dpSubStr(\"SCTmops1:Sector.Row_00.ST_07:_original.._value\",  DPSUB_SYS_DP_EL);
  if ( strpos(sDp,\".\") < 1 )
    sDp += \".\";

  sFormat = dpGetFormat( sDp );
  if( !checkStringFormat(sTmp, sFormat) )
  {
    ChildPanelOnCentral( \"vision/MessageWarning\",
                         getCatStr( \"e_para\", \"warning\" ),
                         makeDynString( getCatStr( \"e_para\", \"wrongFormat\" )));
    return;
  }

  dpSetWait(\"SCTmops1:Sector.Row_00.ST_07:_original.._value\", sTmp);
  err = getLastError();
  if (dynlen(err) > 0)
    errorDialog(err);
}

// SimpleCtrlScript {EP_textFieldOut}
// DP {SCTmops1:Sector.Row_00.ST_00}
// Config {:_original.._value}
// DPType {int}
// SimpleCtrlScriptEnd {EP_textFieldOut}
" 0

E

N 0 100 1 0 0 1
21 965
"SpinButton9"
""
1 30 329 E E E 1 E 1 E N "_WindowText" E N "_Window" E E
 E E
964 0 0 0 0 0
EE E
0
1
LANG:1 0 
0
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
28 327 72 353
0
"// SimpleCtrlScriptStart {valid}
main()
{
  EP_textFieldIn();
  EP_setInvalid();
}

EP_textFieldIn()
{
dyn_errClass err;

  if( dpSubStr( \"SCTmops1:Sector.Row_00.ST_08:_online.._value\", DPSUB_DP_EL ) == \"\" )
  {
    setValue(\"\", \"color\", \"_dpdoesnotexist\");
    return;
  }

  dpConnect(\"EP_textFieldInCB\",
            \"SCTmops1:Sector.Row_00.ST_08:_online.._value\");
  err = getLastError();
  if (dynlen(err) > 0)
    setValue(\"\", \"color\", \"_dpdoesnotexist\");

}

EP_textFieldInCB(string dp, int iNewValue)
{
  setValue(\"\", \"text\", dpValToString(dp, iNewValue, TRUE) );
}

EP_setInvalid()
{
dyn_errClass err;

  if( dpSubStr( \"SCTmops1:Sector.Row_00.ST_00:_online.._invalid\", DPSUB_DP_EL ) == \"\" )
  {
    setValue(\"\", \"color\", \"_dpdoesnotexist\");
    return;
  }

  dpConnect(\"EP_setInvalidCB\",
            \"SCTmops1:Sector.Row_00.ST_00:_online.._invalid\");
  err = getLastError();
  if (dynlen(err) > 0)
    setValue(\"\", \"color\", \"_dpdoesnotexist\");

}

EP_setInvalidCB(string dp, bool boInvalid)
{
  setValue(\"\", \"color\", (boInvalid ? \"_invalid\" : \"\"));
}

// SimpleCtrlScript {EP_textFieldIn}
// DP {SCTmops1:Sector.Row_00.ST_08}
// DPConfig {:_online.._value}
// DPType {int}
// UseDPUnit {TRUE}
// UseDPFormat {TRUE}
// SimpleCtrlScriptEnd {EP_textFieldIn}
// SimpleCtrlScript {EP_setInvalid}
// DP {SCTmops1:Sector.Row_00.ST_00}
// DPConfig {:_online.._invalid}
// DPType {bool}
// Attribut {color}
// SimpleCtrlScriptEnd {EP_setInvalid}
" 0

"// SimpleCtrlScriptStart {invalid}
main()
{
  EP_textFieldOut();
}

EP_textFieldOut()
{
int iNewValue;
dyn_errClass err;
string sTmp;
string sFormat, sDp;

  getValue(\"\", \"text\", sTmp);
  sscanf(sTmp, \"%d\", iNewValue);

  sDp = dpSubStr(\"SCTmops1:Sector.Row_00.ST_08:_original.._value\",  DPSUB_SYS_DP_EL);
  if ( strpos(sDp,\".\") < 1 )
    sDp += \".\";

  sFormat = dpGetFormat( sDp );
  if( !checkStringFormat(sTmp, sFormat) )
  {
    ChildPanelOnCentral( \"vision/MessageWarning\",
                         getCatStr( \"e_para\", \"warning\" ),
                         makeDynString( getCatStr( \"e_para\", \"wrongFormat\" )));
    return;
  }

  dpSetWait(\"SCTmops1:Sector.Row_00.ST_08:_original.._value\", sTmp);
  err = getLastError();
  if (dynlen(err) > 0)
    errorDialog(err);
}

// SimpleCtrlScript {EP_textFieldOut}
// DP {SCTmops1:Sector.Row_00.ST_00}
// Config {:_original.._value}
// DPType {int}
// SimpleCtrlScriptEnd {EP_textFieldOut}
" 0

E

N 0 100 1 0 0 1
21 966
"SpinButton10"
""
1 30 358 E E E 1 E 1 E N "_WindowText" E N "_Window" E E
 E E
965 0 0 0 0 0
EE E
0
1
LANG:1 0 
0
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
28 356 72 382
0
"// SimpleCtrlScriptStart {valid}
main()
{
  EP_textFieldIn();
  EP_setInvalid();
}

EP_textFieldIn()
{
dyn_errClass err;

  if( dpSubStr( \"SCTmops1:Sector.Row_00.ST_09:_online.._value\", DPSUB_DP_EL ) == \"\" )
  {
    setValue(\"\", \"color\", \"_dpdoesnotexist\");
    return;
  }

  dpConnect(\"EP_textFieldInCB\",
            \"SCTmops1:Sector.Row_00.ST_09:_online.._value\");
  err = getLastError();
  if (dynlen(err) > 0)
    setValue(\"\", \"color\", \"_dpdoesnotexist\");

}


EP_textFieldInCB(string dp, int iNewValue)
{
  setValue(\"\", \"text\", iNewValue);
}

EP_setInvalid()
{
dyn_errClass err;

  if( dpSubStr( \"SCTmops1:Sector.Row_00.ST_09:_online.._invalid\", DPSUB_DP_EL ) == \"\" )
  {
    setValue(\"\", \"color\", \"_dpdoesnotexist\");
    return;
  }

  dpConnect(\"EP_setInvalidCB\",
            \"SCTmops1:Sector.Row_00.ST_09:_online.._invalid\");
  err = getLastError();
  if (dynlen(err) > 0)
    setValue(\"\", \"color\", \"_dpdoesnotexist\");

}

EP_setInvalidCB(string dp, bool boInvalid)
{
  setValue(\"\", \"color\", (boInvalid ? \"_invalid\" : \"\"));
}

// SimpleCtrlScript {EP_textFieldIn}
// DP {SCTmops1:Sector.Row_00.ST_09}
// DPConfig {:_online.._value}
// DPType {int}
// UseDPUnit {FALSE}
// UseDPFormat {FALSE}
// SimpleCtrlScriptEnd {EP_textFieldIn}
// SimpleCtrlScript {EP_setInvalid}
// DP {SCTmops1:Sector.Row_00.ST_09}
// DPConfig {:_online.._invalid}
// DPType {bool}
// Attribut {color}
// SimpleCtrlScriptEnd {EP_setInvalid}
" 0

"// SimpleCtrlScriptStart {invalid}
main()
{
  EP_textFieldOut();
}

EP_textFieldOut()
{
int iNewValue;
dyn_errClass err;
string sTmp;
string sFormat, sDp;

  getValue(\"\", \"text\", sTmp);
  sscanf(sTmp, \"%d\", iNewValue);

  sDp = dpSubStr(\"SCTmops1:Sector.Row_00.ST_09:_original.._value\",  DPSUB_SYS_DP_EL);
  if ( strpos(sDp,\".\") < 1 )
    sDp += \".\";

  sFormat = dpGetFormat( sDp );
  if( !checkStringFormat(sTmp, sFormat) )
  {
    ChildPanelOnCentral( \"vision/MessageWarning\",
                         getCatStr( \"e_para\", \"warning\" ),
                         makeDynString( getCatStr( \"e_para\", \"wrongFormat\" )));
    return;
  }

  dpSetWait(\"SCTmops1:Sector.Row_00.ST_09:_original.._value\", sTmp);
  err = getLastError();
  if (dynlen(err) > 0)
    errorDialog(err);
}

// SimpleCtrlScript {EP_textFieldOut}
// DP {SCTmops1:Sector.Row_00.ST_00}
// Config {:_original.._value}
// DPType {int}
// SimpleCtrlScriptEnd {EP_textFieldOut}
" 0

E

N 0 100 1 0 0 1
21 967
"SpinButton11"
""
1 30 387 E E E 1 E 1 E N "_WindowText" E N "_Window" E E
 E E
966 0 0 0 0 0
EE E
0
1
LANG:1 0 
0
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
28 385 72 411
0
"// SimpleCtrlScriptStart {valid}
main()
{
  EP_textFieldIn();
  EP_setInvalid();
}

EP_textFieldIn()
{
dyn_errClass err;

  if( dpSubStr( \"SCTmops1:Sector.Row_00.ST_10:_online.._value\", DPSUB_DP_EL ) == \"\" )
  {
    setValue(\"\", \"color\", \"_dpdoesnotexist\");
    return;
  }

  dpConnect(\"EP_textFieldInCB\",
            \"SCTmops1:Sector.Row_00.ST_10:_online.._value\");
  err = getLastError();
  if (dynlen(err) > 0)
    setValue(\"\", \"color\", \"_dpdoesnotexist\");

}


EP_textFieldInCB(string dp, int iNewValue)
{
  setValue(\"\", \"text\", iNewValue);
}

EP_setInvalid()
{
dyn_errClass err;

  if( dpSubStr( \"SCTmops1:Sector.Row_00.ST_10:_online.._invalid\", DPSUB_DP_EL ) == \"\" )
  {
    setValue(\"\", \"color\", \"_dpdoesnotexist\");
    return;
  }

  dpConnect(\"EP_setInvalidCB\",
            \"SCTmops1:Sector.Row_00.ST_10:_online.._invalid\");
  err = getLastError();
  if (dynlen(err) > 0)
    setValue(\"\", \"color\", \"_dpdoesnotexist\");

}

EP_setInvalidCB(string dp, bool boInvalid)
{
  setValue(\"\", \"color\", (boInvalid ? \"_invalid\" : \"\"));
}

// SimpleCtrlScript {EP_textFieldIn}
// DP {SCTmops1:Sector.Row_00.ST_10}
// DPConfig {:_online.._value}
// DPType {int}
// UseDPUnit {FALSE}
// UseDPFormat {FALSE}
// SimpleCtrlScriptEnd {EP_textFieldIn}
// SimpleCtrlScript {EP_setInvalid}
// DP {SCTmops1:Sector.Row_00.ST_10}
// DPConfig {:_online.._invalid}
// DPType {bool}
// Attribut {color}
// SimpleCtrlScriptEnd {EP_setInvalid}
" 0

"// SimpleCtrlScriptStart {invalid}
main()
{
  EP_textFieldOut();
}

EP_textFieldOut()
{
int iNewValue;
dyn_errClass err;
string sTmp;
string sFormat, sDp;

  getValue(\"\", \"text\", sTmp);
  sscanf(sTmp, \"%d\", iNewValue);

  sDp = dpSubStr(\"SCTmops1:Sector.Row_00.ST_10:_original.._value\",  DPSUB_SYS_DP_EL);
  if ( strpos(sDp,\".\") < 1 )
    sDp += \".\";

  sFormat = dpGetFormat( sDp );
  if( !checkStringFormat(sTmp, sFormat) )
  {
    ChildPanelOnCentral( \"vision/MessageWarning\",
                         getCatStr( \"e_para\", \"warning\" ),
                         makeDynString( getCatStr( \"e_para\", \"wrongFormat\" )));
    return;
  }

  dpSetWait(\"SCTmops1:Sector.Row_00.ST_10:_original.._value\", sTmp);
  err = getLastError();
  if (dynlen(err) > 0)
    errorDialog(err);
}

// SimpleCtrlScript {EP_textFieldOut}
// DP {SCTmops1:Sector.Row_00.ST_00}
// Config {:_original.._value}
// DPType {int}
// SimpleCtrlScriptEnd {EP_textFieldOut}
" 0

E

N 0 100 1 0 0 1
21 968
"SpinButton12"
""
1 30 416 E E E 1 E 1 E N "_WindowText" E N "_Window" E E
 E E
967 0 0 0 0 0
EE E
0
1
LANG:1 0 
0
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
28 414 72 440
0
"// SimpleCtrlScriptStart {valid}
main()
{
  EP_textFieldIn();
  EP_setInvalid();
}

EP_textFieldIn()
{
dyn_errClass err;

  if( dpSubStr( \"SCTmops1:Sector.Row_00.ST_11:_online.._value\", DPSUB_DP_EL ) == \"\" )
  {
    setValue(\"\", \"color\", \"_dpdoesnotexist\");
    return;
  }

  dpConnect(\"EP_textFieldInCB\",
            \"SCTmops1:Sector.Row_00.ST_11:_online.._value\");
  err = getLastError();
  if (dynlen(err) > 0)
    setValue(\"\", \"color\", \"_dpdoesnotexist\");

}


EP_textFieldInCB(string dp, int iNewValue)
{
  setValue(\"\", \"text\", iNewValue);
}

EP_setInvalid()
{
dyn_errClass err;

  if( dpSubStr( \"SCTmops1:Sector.Row_00.ST_11:_online.._invalid\", DPSUB_DP_EL ) == \"\" )
  {
    setValue(\"\", \"color\", \"_dpdoesnotexist\");
    return;
  }

  dpConnect(\"EP_setInvalidCB\",
            \"SCTmops1:Sector.Row_00.ST_11:_online.._invalid\");
  err = getLastError();
  if (dynlen(err) > 0)
    setValue(\"\", \"color\", \"_dpdoesnotexist\");

}

EP_setInvalidCB(string dp, bool boInvalid)
{
  setValue(\"\", \"color\", (boInvalid ? \"_invalid\" : \"\"));
}

// SimpleCtrlScript {EP_textFieldIn}
// DP {SCTmops1:Sector.Row_00.ST_11}
// DPConfig {:_online.._value}
// DPType {int}
// UseDPUnit {FALSE}
// UseDPFormat {FALSE}
// SimpleCtrlScriptEnd {EP_textFieldIn}
// SimpleCtrlScript {EP_setInvalid}
// DP {SCTmops1:Sector.Row_00.ST_11}
// DPConfig {:_online.._invalid}
// DPType {bool}
// Attribut {color}
// SimpleCtrlScriptEnd {EP_setInvalid}
" 0

"// SimpleCtrlScriptStart {invalid}
main()
{
  EP_textFieldOut();
}

EP_textFieldOut()
{
int iNewValue;
dyn_errClass err;
string sTmp;
string sFormat, sDp;

  getValue(\"\", \"text\", sTmp);
  sscanf(sTmp, \"%d\", iNewValue);

  sDp = dpSubStr(\"SCTmops1:Sector.Row_00.ST_11:_original.._value\",  DPSUB_SYS_DP_EL);
  if ( strpos(sDp,\".\") < 1 )
    sDp += \".\";

  sFormat = dpGetFormat( sDp );
  if( !checkStringFormat(sTmp, sFormat) )
  {
    ChildPanelOnCentral( \"vision/MessageWarning\",
                         getCatStr( \"e_para\", \"warning\" ),
                         makeDynString( getCatStr( \"e_para\", \"wrongFormat\" )));
    return;
  }

  dpSetWait(\"SCTmops1:Sector.Row_00.ST_11:_original.._value\", sTmp);
  err = getLastError();
  if (dynlen(err) > 0)
    errorDialog(err);
}

// SimpleCtrlScript {EP_textFieldOut}
// DP {SCTmops1:Sector.Row_00.ST_00}
// Config {:_original.._value}
// DPType {int}
// SimpleCtrlScriptEnd {EP_textFieldOut}
" 0

E

N 0 100 1 0 0 1
21 969
"SpinButton13"
""
1 30 97 E E E 1 E 1 E N "_WindowText" E N "_Window" E E
 E E
968 0 0 0 0 0
EE E
0
1
LANG:1 0 
0
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
28 95 72 121
0
"// SimpleCtrlScriptStart {invalid}
main()
{
  EP_textFieldIn();
  EP_setInvalid();
}

EP_textFieldIn()
{
dyn_errClass err;

  if( dpSubStr( \"SCTmops1:Sector.Row_00.ST_00:_online.._value\", DPSUB_DP_EL ) == \"\" )
  {
    setValue(\"\", \"color\", \"_dpdoesnotexist\");
    return;
  }

  dpConnect(\"EP_textFieldInCB\",
            \"SCTmops1:Sector.Row_00.ST_00:_online.._value\");
  err = getLastError();
  if (dynlen(err) > 0)
    setValue(\"\", \"color\", \"_dpdoesnotexist\");

}


EP_textFieldInCB(string dp, int iNewValue)
{
  setValue(\"\", \"text\", dpValToString(dp, iNewValue, TRUE) );
}

EP_setInvalid()
{
dyn_errClass err;

  if( dpSubStr( \"SCTmops1:Sector.Row_00.ST_00:_online.._invalid\", DPSUB_DP_EL ) == \"\" )
  {
    setValue(\"\", \"color\", \"_dpdoesnotexist\");
    return;
  }

  dpConnect(\"EP_setInvalidCB\",
            \"SCTmops1:Sector.Row_00.ST_00:_online.._invalid\");
  err = getLastError();
  if (dynlen(err) > 0)
    setValue(\"\", \"color\", \"_dpdoesnotexist\");

}

EP_setInvalidCB(string dp, bool boInvalid)
{
  setValue(\"\", \"color\", (boInvalid ? \"_invalid\" : \"\"));
}

// SimpleCtrlScript {EP_textFieldIn}
// DP {SCTmops1:Sector.Row_00.ST_00}
// DPConfig {:_online.._value}
// DPType {int}
// UseDPUnit {TRUE}
// UseDPFormat {TRUE}
// SimpleCtrlScriptEnd {EP_textFieldIn}
// SimpleCtrlScript {EP_setInvalid}
// DP {SCTmops1:Sector.Row_00.ST_00}
// DPConfig {:_online.._invalid}
// DPType {bool}
// Attribut {color}
// SimpleCtrlScriptEnd {EP_setInvalid}
" 0

"// SimpleCtrlScriptStart {valid}
main()
{
  EP_textFieldOut();
}

EP_textFieldOut()
{
int iNewValue;
dyn_errClass err;
string sTmp;
string sFormat, sDp;

  getValue(\"\", \"text\", sTmp);
  sscanf(sTmp, \"%d\", iNewValue);

  sDp = dpSubStr(\"SCTmops1:Sector.Row_00.ST_00:_original.._value\",  DPSUB_SYS_DP_EL);
  if ( strpos(sDp,\".\") < 1 )
    sDp += \".\";

  sFormat = dpGetFormat( sDp );
  if( !checkStringFormat(sTmp, sFormat) )
  {
    ChildPanelOnCentral( \"vision/MessageWarning\",
                         getCatStr( \"e_para\", \"warning\" ),
                         makeDynString( getCatStr( \"e_para\", \"wrongFormat\" )));
    return;
  }

  dpSetWait(\"SCTmops1:Sector.Row_00.ST_00:_original.._value\", sTmp);
  err = getLastError();
  if (dynlen(err) > 0)
    errorDialog(err);
}

// SimpleCtrlScript {EP_textFieldOut}
// DP {SCTmops1:Sector.Row_00.ST_00}
// Config {:_original.._value}
// DPType {int}
// SimpleCtrlScriptEnd {EP_textFieldOut}
" 0

E

N 0 100 1 0 0 1
21 970
"SpinButton14"
""
1 30 126 E E E 1 E 1 E N "_WindowText" E N "_Window" E E
 E E
969 0 0 0 0 0
EE E
0
1
LANG:1 0 
0
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
28 124 72 150
0
"// SimpleCtrlScriptStart {valid}
main()
{
  EP_textFieldIn();
  EP_setInvalid();
}

EP_textFieldIn()
{
dyn_errClass err;

  if( dpSubStr( \"SCTmops1:Sector.Row_00.ST_01:_online.._value\", DPSUB_DP_EL ) == \"\" )
  {
    setValue(\"\", \"color\", \"_dpdoesnotexist\");
    return;
  }

  dpConnect(\"EP_textFieldInCB\",
            \"SCTmops1:Sector.Row_00.ST_01:_online.._value\");
  err = getLastError();
  if (dynlen(err) > 0)
    setValue(\"\", \"color\", \"_dpdoesnotexist\");

}


EP_textFieldInCB(string dp, int iNewValue)
{
  setValue(\"\", \"text\", iNewValue);
}

EP_setInvalid()
{
dyn_errClass err;

  if( dpSubStr( \"SCTmops1:Sector.Row_00.ST_01:_online.._invalid\", DPSUB_DP_EL ) == \"\" )
  {
    setValue(\"\", \"color\", \"_dpdoesnotexist\");
    return;
  }

  dpConnect(\"EP_setInvalidCB\",
            \"SCTmops1:Sector.Row_00.ST_01:_online.._invalid\");
  err = getLastError();
  if (dynlen(err) > 0)
    setValue(\"\", \"color\", \"_dpdoesnotexist\");

}

EP_setInvalidCB(string dp, bool boInvalid)
{
  setValue(\"\", \"color\", (boInvalid ? \"_invalid\" : \"\"));
}

// SimpleCtrlScript {EP_textFieldIn}
// DP {SCTmops1:Sector.Row_00.ST_01}
// DPConfig {:_online.._value}
// DPType {int}
// UseDPUnit {FALSE}
// UseDPFormat {FALSE}
// SimpleCtrlScriptEnd {EP_textFieldIn}
// SimpleCtrlScript {EP_setInvalid}
// DP {SCTmops1:Sector.Row_00.ST_01}
// DPConfig {:_online.._invalid}
// DPType {bool}
// Attribut {color}
// SimpleCtrlScriptEnd {EP_setInvalid}
" 0

"// SimpleCtrlScriptStart {invalid}
main()
{
  EP_textFieldOut();
}

EP_textFieldOut()
{
int iNewValue;
dyn_errClass err;
string sTmp;
string sFormat, sDp;

  getValue(\"\", \"text\", sTmp);
  sscanf(sTmp, \"%d\", iNewValue);

  sDp = dpSubStr(\"SCTmops1:Sector.Row_00.ST_01:_original.._value\",  DPSUB_SYS_DP_EL);
  if ( strpos(sDp,\".\") < 1 )
    sDp += \".\";

  sFormat = dpGetFormat( sDp );
  if( !checkStringFormat(sTmp, sFormat) )
  {
    ChildPanelOnCentral( \"vision/MessageWarning\",
                         getCatStr( \"e_para\", \"warning\" ),
                         makeDynString( getCatStr( \"e_para\", \"wrongFormat\" )));
    return;
  }

  dpSetWait(\"SCTmops1:Sector.Row_00.ST_01:_original.._value\", sTmp);
  err = getLastError();
  if (dynlen(err) > 0)
    errorDialog(err);
}

// SimpleCtrlScript {EP_textFieldOut}
// DP {SCTmops1:Sector.Row_00.ST_00}
// Config {:_original.._value}
// DPType {int}
// SimpleCtrlScriptEnd {EP_textFieldOut}
" 0

E

N 0 100 1 0 0 1
21 971
"SpinButton15"
""
1 30 155 E E E 1 E 1 E N "_WindowText" E N "_Window" E E
 E E
970 0 0 0 0 0
EE E
0
1
LANG:1 0 
0
1
LANG:1 119 -microsoft windows-Courier New-normal-r-normal-*-*-110-100-100-*-*-iso8859-1|-12,0,0,0,400,0,0,0,0,3,2,1,49,Courier New
0 ""
28 153 72 179
0
"// SimpleCtrlScriptStart {valid}
main()
{
  EP_textFieldIn();
  EP_setInvalid();
}

EP_textFieldIn()
{
dyn_errClass err;

  if( dpSubStr( \"SCTmops1:Sector.Row_00.ST_02:_online.._value\", DPSUB_DP_EL ) == \"\" )
  {
    setValue(\"\", \"color\", \"_dpdoesnotexist\");
    return;
  }

  dpConnect(\"EP_textFieldInCB\",
            \"SCTmops1:Sector.Row_00.ST_02:_online.._value\");
  err = getLastError();
  if (dynlen(err) > 0)
    setValue(\"\", \"color\", \"_dpdoesnotexist\");

}


EP_textFieldInCB(string dp, int iNewValue)
{
  setValue(\"\", \"text\", dpValToString(dp, iNewValue, TRUE) );
}

EP_setInvalid()
{
dyn_errClass err;

  if( dpSubStr( \"SCTmops1:Sector.Row_00.ST_02:_online.._invalid\", DPSUB_DP_EL ) == \"\" )
  {
    setValue(\"\", \"color\", \"_dpdoesnotexist\");
    return;
  }

  dpConnect(\"EP_setInvalidCB\",
            \"SCTmops1:Sector.Row_00.ST_02:_online.._invalid\");
  err = getLastError();
  if (dynlen(err) > 0)
    setValue(\"\", \"color\", \"_dpdoesnotexist\");

}

EP_setInvalidCB(string dp, bool boInvalid)
{
  setValue(\"\", \"color\", (boInvalid ? \"_invalid\" : \"\"));
}

// SimpleCtrlScript {EP_textFieldIn}
// DP {SCTmops1:Sector.Row_00.ST_02}
// DPConfig {:_online.._value}
// DPType {int}
// UseDPUnit {TRUE}
// UseDPFormat {TRUE}
// SimpleCtrlScriptEnd {EP_textFieldIn}
// SimpleCtrlScript {EP_setInvalid}
// DP {SCTmops1:Sector.Row_00.ST_02}
// DPConfig {:_online.._invalid}
// DPType {bool}
// Attribut {color}
// SimpleCtrlScriptEnd {EP_setInvalid}
" 0

"// SimpleCtrlScriptStart {invalid}
main()
{
  EP_textFieldOut();
}

EP_textFieldOut()
{
int iNewValue;
dyn_errClass err;
string sTmp;
string sFormat, sDp;

  getValue(\"\", \"text\", sTmp);
  sscanf(sTmp, \"%d\", iNewValue);

  sDp = dpSubStr(\"SCTmops1:Sector.Row_00.ST_02:_original.._value\",  DPSUB_SYS_DP_EL);
  if ( strpos(sDp,\".\") < 1 )
    sDp += \".\";

  sFormat = dpGetFormat( sDp );
  if( !checkStringFormat(sTmp, sFormat) )
  {
    ChildPanelOnCentral( \"vision/MessageWarning\",
                         getCatStr( \"e_para\", \"warning\" ),
                         makeDynString( getCatStr( \"e_para\", \"wrongFormat\" )));
    return;
  }

  dpSetWait(\"SCTmops1:Sector.Row_00.ST_02:_original.._value\", sTmp);
  err = getLastError();
  if (dynlen(err) > 0)
    errorDialog(err);
}

// SimpleCtrlScript {EP_textFieldOut}
// DP {SCTmops1:Sector.Row_00.ST_00}
// Config {:_original.._value}
// DPType {int}
// SimpleCtrlScriptEnd {EP_textFieldOut}
" 0

E

N 0 100 1 0 0 1
0
LAYER, 1 
1
LANG:1 6 Layer2
0
LAYER, 2 
1
LANG:1 6 Layer3
0
LAYER, 3 
1
LANG:1 6 Layer4
0
LAYER, 4 
1
LANG:1 6 Layer5
0
LAYER, 5 
1
LANG:1 6 Layer6
0
LAYER, 6 
1
LANG:1 6 Layer7
0
LAYER, 7 
1
LANG:1 6 Layer8
0
0