Far Detector PMT Linearity Update

Pat Ward University of Cambridge

• At last meeting fitted each strip-end against all other strip-ends for the

same LED using Far data (June 2005 gain curve)

⇒ good fits for ∼98% of strip-ends ⇒ PMTs are linear in region 200 < ADC < 7000

But how linear?

• Could perform linearity correction by fitting Near v Far data for each strip,

but 13% of strip-ends have < 3 Near points in linear region

Far-Far Linearity Plots • Have redone fits to Far data, but fitted each strip-end against MEAN of all

GOOD strip-ends for that LED

• Average all strip-ends with 1000 < max(ADC) < 6000 • Fit each strip-end against mean in range 200 < ADC < 7000 • Remove strip-ends with npfit < 5 or χ^2/dof > 2 • Make new averages and redo fits • Iterate 3 times • Approx. 80% of strips are included in averages • Mean number of good strips per LED = 474 • Minimum number of good strips per LED = 52

PulserBox 6 LED 2: 368 strip-ends have max(ADC) > 6000

Far-Far: Fit χ2 Values

• Fits generally reason-

able

• 98% of strip-ends have χ^2/dof < 10 • 96% of strip-ends have χ^2/dof < 3 • < χ^2/dof >= 1.35 (excluding values

> 10)

Far-Far Fits • Fits generally reasonable, but χ^2 values tend to be larger than for fits to a

single strip-end Errors on mean values smaller

• Several channels show signs of saturation at ADC values of ∼ 5000 (e.g.

example 2)

• Try to quantify linearity by calculating residuals from fitted line • Plot mean residual v. strip-end ADC value for good strips (χ^2/dof < 2) • Find distinct systematic deviations from linearity

Far-Far Fit Residuals

Far-Far Fit Residuals

• For good strip-ends,

mean absolute value of residuals in fit range = 0.61%

• 99% of good strip-ends

have value < 1%

• Linearity good enough?

Near-Far Linearity Plots • Have also fitted Near data to MEAN of all GOOD Far strip-ends for that LED

Straight line in 200 < ADC < 7000

• Again see effect of smaller er-

rors on means

• While many strip-ends give

good χ^2, a significant fraction which do not

• For the 82% of strip-ends with

at least 3 points in fit range, <

χ^2/dof >= 2.11 (excluding

those >10)

Near-Far Fits • Have tried fitting Near data to mean Far data for that led using Giles’s

‘Pole+Kicker’ function:

• Fit to straight line in range 200 < ADC < 7000 • Using slope from first fit to give starting value for that parameter, fit to

Pole (3 parameters) function in range ADC > 200

• Using results of second fit to give starting values, fit to Pole+Kicker (5

parameters) function in range ADC > 200

• Problem: points near saturation limit have very small errors:

⇒ set any error <0.2% to 0.2% • Second and third fits change slope from first fit by ≤ 0.7% • Pole alone does not give good fits, pole+kicker gives reasonable fits • Increasing lower limit on fit range to 500 gives small improvement in χ^2/dof

Near-Far Fit: example 1

Near-Far Fit χ2

Near-Far Fit Residuals

Near-Far Fit Residuals

• Mean absolute value of

residuals = 0.23%

• 99.5% of strip-ends

have value < 1%

Near-Far Linearity Plots • At last meeting it was suggested that all spots on same pixel should show

similar behaviour, so could use another spot on same pixel for channels with too few points in linear region

• Have investigated using Near v. mean Far straight-line fits (in 200 < ADC < 7000) • Calculate fit residuals as function of Near ADC, and compare spots on

same pixel

• See good correlation ⇒ should be possible to use neighbouring spot for

channel with bad fit, but need to quantify agreement

Near-Far Fit Residuals

Near-Far Fit Residuals

Summary • Have redone linear fits of Far data to mean of ‘good’ strip-ends for that LED • The χ^2 values are larger than for fits to a single strip-end, but probably

acceptable

• See systematic effects in the residuals, but these at a level <1% • Near data can be fitted to Far means using ‘Pole+kicker’ function’ • Mean residuals typically ∼0.2%, and 99.5% of channels <1% • Have compared straight-line fit residuals for spots on same pixel • See good correlation ⇒ can probably use neighbouring spot for bad

channels